(kicad_sch (version 20220126) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "74xx:74HC164" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 1.905 -13.97 0))
      (property "Value" "74HC164" (id 1) (at 1.905 -16.51 0))
      (property "Footprint" "" (id 2) (at 22.86 -7.62 0))
      (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT164.pdf" (id 3) (at 22.86 -7.62 0))
      (property "ki_keywords" "8-bit shift register" (id 4) (at 0 0 0))
      (property "ki_description" "8-bit serial-in parallel-out shift register" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x8.7*P1.27mm* ?SSOP*P0.65mm* DIP*W7.62mm*" (id 6) (at 0 0 0))
      (symbol "74HC164_0_1"
        (rectangle (start 7.62 10.16) (end -7.62 -12.7)
          (fill (type background))
        )
      )
      (symbol "74HC164_1_1"
        (pin input line (at -10.16 0 0) (length 2.54)
          (name "DSA")
          (number "1")
        )
        (pin output line (at 10.16 -2.54 180) (length 2.54)
          (name "Q4")
          (number "10")
        )
        (pin output line (at 10.16 -5.08 180) (length 2.54)
          (name "Q5")
          (number "11")
        )
        (pin output line (at 10.16 -7.62 180) (length 2.54)
          (name "Q6")
          (number "12")
        )
        (pin output line (at 10.16 -10.16 180) (length 2.54)
          (name "Q7")
          (number "13")
        )
        (pin power_in line (at 0 12.7 270) (length 2.54)
          (name "VCC")
          (number "14")
        )
        (pin input line (at -10.16 -2.54 0) (length 2.54)
          (name "DSB")
          (number "2")
        )
        (pin output line (at 10.16 7.62 180) (length 2.54)
          (name "Q0")
          (number "3")
        )
        (pin output line (at 10.16 5.08 180) (length 2.54)
          (name "Q1")
          (number "4")
        )
        (pin output line (at 10.16 2.54 180) (length 2.54)
          (name "Q2")
          (number "5")
        )
        (pin output line (at 10.16 0 180) (length 2.54)
          (name "Q3")
          (number "6")
        )
        (pin power_in line (at 0 -15.24 90) (length 2.54)
          (name "GND")
          (number "7")
        )
        (pin input line (at -10.16 -7.62 0) (length 2.54)
          (name "CP")
          (number "8")
        )
        (pin input line (at -10.16 5.08 0) (length 2.54)
          (name "~{MR}")
          (number "9")
        )
      )
    )
    (symbol "74xx:74LS245" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -7.62 16.51 0))
      (property "Value" "74LS245" (id 1) (at -7.62 -16.51 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "TTL BUS 3State" (id 5) (at 0 0 0))
      (property "ki_description" "Octal BUS Transceivers, 3-State outputs" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP?20*" (id 7) (at 0 0 0))
      (symbol "74LS245_1_0"
        (polyline
          (pts
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy 0.635 -1.27)
            (xy 0.635 1.27)
            (xy 1.27 1.27)
          )
          (fill (type none))
        )
        (pin input line (at -12.7 -10.16 0) (length 5.08)
          (name "A->B")
          (number "1")
        )
        (pin power_in line (at 0 -20.32 90) (length 5.08)
          (name "GND")
          (number "10")
        )
        (pin tri_state line (at 12.7 -5.08 180) (length 5.08)
          (name "B7")
          (number "11")
        )
        (pin tri_state line (at 12.7 -2.54 180) (length 5.08)
          (name "B6")
          (number "12")
        )
        (pin tri_state line (at 12.7 0 180) (length 5.08)
          (name "B5")
          (number "13")
        )
        (pin tri_state line (at 12.7 2.54 180) (length 5.08)
          (name "B4")
          (number "14")
        )
        (pin tri_state line (at 12.7 5.08 180) (length 5.08)
          (name "B3")
          (number "15")
        )
        (pin tri_state line (at 12.7 7.62 180) (length 5.08)
          (name "B2")
          (number "16")
        )
        (pin tri_state line (at 12.7 10.16 180) (length 5.08)
          (name "B1")
          (number "17")
        )
        (pin tri_state line (at 12.7 12.7 180) (length 5.08)
          (name "B0")
          (number "18")
        )
        (pin input inverted (at -12.7 -12.7 0) (length 5.08)
          (name "CE")
          (number "19")
        )
        (pin tri_state line (at -12.7 12.7 0) (length 5.08)
          (name "A0")
          (number "2")
        )
        (pin power_in line (at 0 20.32 270) (length 5.08)
          (name "VCC")
          (number "20")
        )
        (pin tri_state line (at -12.7 10.16 0) (length 5.08)
          (name "A1")
          (number "3")
        )
        (pin tri_state line (at -12.7 7.62 0) (length 5.08)
          (name "A2")
          (number "4")
        )
        (pin tri_state line (at -12.7 5.08 0) (length 5.08)
          (name "A3")
          (number "5")
        )
        (pin tri_state line (at -12.7 2.54 0) (length 5.08)
          (name "A4")
          (number "6")
        )
        (pin tri_state line (at -12.7 0 0) (length 5.08)
          (name "A5")
          (number "7")
        )
        (pin tri_state line (at -12.7 -2.54 0) (length 5.08)
          (name "A6")
          (number "8")
        )
        (pin tri_state line (at -12.7 -5.08 0) (length 5.08)
          (name "A7")
          (number "9")
        )
      )
      (symbol "74LS245_1_1"
        (rectangle (start -7.62 15.24) (end 7.62 -15.24)
          (fill (type background))
        )
      )
    )
    (symbol "Amplifier_Audio:LM386" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 1.27 7.62 0))
      (property "Value" "LM386" (id 1) (at 1.27 5.08 0))
      (property "Footprint" "" (id 2) (at 2.54 2.54 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm386.pdf" (id 3) (at 5.08 5.08 0))
      (property "ki_keywords" "single Power opamp" (id 4) (at 0 0 0))
      (property "ki_description" "Low Voltage Audio Power Amplifier, DIP-8/SOIC-8/SSOP-8" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* MSSOP*P0.65mm* TSSOP*3x3mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "LM386_0_1"
        (polyline
          (pts
            (xy 5.08 0)
            (xy -5.08 5.08)
            (xy -5.08 -5.08)
            (xy 5.08 0)
          )
          (fill (type background))
        )
      )
      (symbol "LM386_1_1"
        (pin input line (at 0 -7.62 90) (length 5.08)
          (name "GAIN")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "2")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "3")
        )
        (pin power_in line (at -2.54 -7.62 90) (length 3.81)
          (name "GND")
          (number "4")
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "5")
        )
        (pin power_in line (at -2.54 7.62 270) (length 3.81)
          (name "V+")
          (number "6")
        )
        (pin input line (at 0 7.62 270) (length 5.08)
          (name "BYPASS")
          (number "7")
        )
        (pin input line (at 2.54 -7.62 90) (length 6.35)
          (name "GAIN")
          (number "8")
        )
      )
    )
    (symbol "Amplifier_Operational:LM2904" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 5.08 0))
      (property "Value" "LM2904" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm358.pdf" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "dual opamp" (id 5) (at 0 0 0))
      (property "ki_description" "Dual Operational Amplifiers, DIP-8/SOIC-8/TSSOP-8/VSSOP-8" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*" (id 7) (at 0 0 0))
      (symbol "LM2904_1_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "2")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "3")
        )
      )
      (symbol "LM2904_2_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "5")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "6")
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "7")
        )
      )
      (symbol "LM2904_3_1"
        (pin power_in line (at -2.54 -7.62 90) (length 3.81)
          (name "V-")
          (number "4")
        )
        (pin power_in line (at -2.54 7.62 270) (length 3.81)
          (name "V+")
          (number "8")
        )
      )
    )
    (symbol "Connector:AudioJack3_Ground_SwitchTR" (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 8.89 0))
      (property "Value" "AudioJack3_Ground_SwitchTR" (id 1) (at 0 6.35 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "audio jack receptacle stereo headphones phones TRS connector" (id 4) (at 0 0 0))
      (property "ki_description" "Audio Jack, 3 Poles (Stereo / TRS), Grounded Sleeve, Switched TR Poles (Normalling)" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Jack*" (id 6) (at 0 0 0))
      (symbol "AudioJack3_Ground_SwitchTR_0_1"
        (rectangle (start -5.08 -5.08) (end -6.35 -7.62)
          (fill (type outline))
        )
        (polyline
          (pts
            (xy 0.508 -0.254)
            (xy 0.762 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.778 -5.334)
            (xy 2.032 -5.842)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -5.08)
            (xy 0.635 -5.715)
            (xy 1.27 -5.08)
            (xy 2.54 -5.08)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -7.62)
            (xy 1.778 -7.62)
            (xy 1.778 -5.334)
            (xy 1.524 -5.842)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 -2.54)
            (xy 0.508 -2.54)
            (xy 0.508 -0.254)
            (xy 0.254 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.905 -5.08)
            (xy -1.27 -5.715)
            (xy -0.635 -5.08)
            (xy -0.635 0)
            (xy 2.54 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 2.54)
            (xy -2.54 2.54)
            (xy -2.54 -5.08)
            (xy -3.175 -5.715)
            (xy -3.81 -5.08)
          )
          (fill (type none))
        )
        (rectangle (start 2.54 3.81) (end -5.08 -10.16)
          (fill (type background))
        )
      )
      (symbol "AudioJack3_Ground_SwitchTR_1_1"
        (pin passive line (at 0 -12.7 90) (length 2.54)
          (name "~")
          (number "G")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "~")
          (number "R")
        )
        (pin passive line (at 5.08 -2.54 180) (length 2.54)
          (name "~")
          (number "RN")
        )
        (pin passive line (at 5.08 2.54 180) (length 2.54)
          (name "~")
          (number "S")
        )
        (pin passive line (at 5.08 -5.08 180) (length 2.54)
          (name "~")
          (number "T")
        )
        (pin passive line (at 5.08 -7.62 180) (length 2.54)
          (name "~")
          (number "TN")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:CP1" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "CP1" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor, US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "CP1_0_1"
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 2.286)
            (xy -0.762 2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.778)
            (xy -1.27 2.794)
          )
          (fill (type none))
        )
        (arc (start 2.032 -1.27) (mid 0 -0.5572) (end -2.032 -1.27)
          (fill (type none))
        )
      )
      (symbol "CP1_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 3.302)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:CP1_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "CP1_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor, small US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "CP1_Small_0_1"
        (polyline
          (pts
            (xy -1.524 0.508)
            (xy 1.524 0.508)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.524)
            (xy -0.762 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.27)
            (xy -1.016 1.778)
          )
          (fill (type none))
        )
        (arc (start 1.524 -0.762) (mid 0 -0.3734) (end -1.524 -0.762)
          (fill (type none))
        )
      )
      (symbol "CP1_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 2.032)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 2.032)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:CP_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.254 1.778 0))
      (property "Value" "CP_Small" (id 1) (at 0.254 -2.032 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Polarized capacitor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "CP_*" (id 6) (at 0 0 0))
      (symbol "CP_Small_0_1"
        (rectangle (start -1.524 -0.3048) (end 1.524 -0.6858)
          (fill (type outline))
        )
        (rectangle (start -1.524 0.6858) (end 1.524 0.3048)
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 1.524)
            (xy -0.762 1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.016 1.27)
            (xy -1.016 1.778)
          )
          (fill (type none))
        )
      )
      (symbol "CP_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 1.8542)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.8542)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Jumper_NC_Small" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.032 0))
      (property "Value" "Jumper_NC_Small" (id 1) (at 0.254 -1.524 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "jumper link bridge NC" (id 4) (at 0 0 0))
      (property "ki_description" "Jumper, normally closed, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SolderJumper*Bridged* Jumper* TestPoint*2Pads* TestPoint*Bridge*" (id 6) (at 0 0 0))
      (symbol "Jumper_NC_Small_0_1"
        (circle (center -1.016 0) (radius 0.508)
          (fill (type none))
        )
        (arc (start -1.016 0.762) (mid 0 -1.6908) (end 1.016 0.762)
          (fill (type none))
        )
        (circle (center 1.016 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -2.54 0 0) (length 1.016)
          (name "1")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 1.016)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:Jumper_NO_Small" (pin_numbers hide) (pin_names (offset 0.762) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.032 0))
      (property "Value" "Jumper_NO_Small" (id 1) (at 0.254 -1.524 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "jumper link bridge NO" (id 4) (at 0 0 0))
      (property "ki_description" "Jumper, normally open, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "SolderJumper*Open* Jumper* TestPoint*2Pads* TestPoint*Bridge*" (id 6) (at 0 0 0))
      (symbol "Jumper_NO_Small_0_1"
        (circle (center -1.016 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 1.016 0) (radius 0.508)
          (fill (type none))
        )
        (pin passive line (at -2.54 0 0) (length 1.016)
          (name "1")
          (number "1")
        )
        (pin passive line (at 2.54 0 180) (length 1.016)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Device:L_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "L" (id 0) (at 0.762 1.016 0))
      (property "Value" "L_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "inductor choke coil reactor magnetic" (id 4) (at 0 0 0))
      (property "ki_description" "Inductor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Choke_* *Coil* Inductor_* L_*" (id 6) (at 0 0 0))
      (symbol "L_Small_0_1"
        (arc (start 0 -1.016) (mid -0.5058 -1.524) (end 0 -2.032)
          (fill (type none))
        )
        (arc (start 0 0) (mid -0.5058 -0.508) (end 0 -1.016)
          (fill (type none))
        )
        (arc (start 0 1.016) (mid -0.5058 0.508) (end 0 0)
          (fill (type none))
        )
        (arc (start 0 2.032) (mid -0.5058 1.524) (end 0 1.016)
          (fill (type none))
        )
      )
      (symbol "L_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.508)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.508)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_POT" (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "RV" (id 0) (at -4.445 0 90))
      (property "Value" "R_POT" (id 1) (at -2.54 0 90))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "resistor variable" (id 4) (at 0 0 0))
      (property "ki_description" "Potentiometer" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Potentiometer*" (id 6) (at 0 0 0))
      (symbol "R_POT_0_1"
        (polyline
          (pts
            (xy 2.54 0)
            (xy 1.524 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.143 0)
            (xy 2.286 0.508)
            (xy 2.286 -0.508)
            (xy 1.143 0)
          )
          (fill (type outline))
        )
        (rectangle (start 1.016 2.54) (end -1.016 -2.54)
          (fill (type none))
        )
      )
      (symbol "R_POT_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "1")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 1.27)
          (name "2")
          (number "2")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "3")
          (number "3")
        )
      )
    )
    (symbol "Device:R_Small" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_0_1"
        (rectangle (start -0.762 1.778) (end 0.762 -1.778)
          (fill (type none))
        )
      )
      (symbol "R_Small_1_1"
        (pin passive line (at 0 2.54 270) (length 0.762)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 0.762)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Small_US" (pin_numbers hide) (pin_names (offset 0.254) hide) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 0.762 0.508 0))
      (property "Value" "R_Small_US" (id 1) (at 0.762 -1.016 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "r resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, small US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Small_US_1_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 1.016 -0.381)
            (xy 0 -0.762)
            (xy -1.016 -1.143)
            (xy 0 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 1.524)
            (xy 1.016 1.143)
            (xy 0 0.762)
            (xy -1.016 0.381)
            (xy 0 0)
          )
          (fill (type none))
        )
        (pin passive line (at 0 2.54 270) (length 1.016)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -2.54 90) (length 1.016)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_US" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.54 0 90))
      (property "Value" "R_US" (id 1) (at -2.54 0 90))
      (property "Footprint" "" (id 2) (at 1.016 -0.254 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor, US symbol" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_US_0_1"
        (polyline
          (pts
            (xy 0 -2.286)
            (xy 0 -2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -0.762)
            (xy 1.016 -1.143)
            (xy 0 -1.524)
            (xy -1.016 -1.905)
            (xy 0 -2.286)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0.762)
            (xy 1.016 0.381)
            (xy 0 0)
            (xy -1.016 -0.381)
            (xy 0 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.286)
            (xy 1.016 1.905)
            (xy 0 1.524)
            (xy -1.016 1.143)
            (xy 0 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "R_US_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:Speaker" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "LS" (id 0) (at 1.27 5.715 0))
      (property "Value" "Speaker" (id 1) (at 1.27 3.81 0))
      (property "Footprint" "" (id 2) (at 0 -5.08 0))
      (property "Datasheet" "~" (id 3) (at -0.254 -1.27 0))
      (property "ki_keywords" "speaker sound" (id 4) (at 0 0 0))
      (property "ki_description" "Speaker" (id 5) (at 0 0 0))
      (symbol "Speaker_0_0"
        (rectangle (start -2.54 1.27) (end 1.016 -3.81)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.016 1.27)
            (xy 3.556 3.81)
            (xy 3.556 -6.35)
            (xy 1.016 -3.81)
          )
          (fill (type none))
        )
      )
      (symbol "Speaker_1_1"
        (pin input line (at -5.08 0 0) (length 2.54)
          (name "1")
          (number "1")
        )
        (pin input line (at -5.08 -2.54 0) (length 2.54)
          (name "2")
          (number "2")
        )
      )
    )
    (symbol "Jumper:Jumper_2_Open" (pin_names (offset 0) hide) (in_bom yes) (on_board yes)
      (property "Reference" "JP" (id 0) (at 0 2.794 0))
      (property "Value" "Jumper_2_Open" (id 1) (at 0 -2.286 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "Jumper SPST" (id 4) (at 0 0 0))
      (property "ki_description" "Jumper, 2-pole, open" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*" (id 6) (at 0 0 0))
      (symbol "Jumper_2_Open_0_0"
        (circle (center -2.032 0) (radius 0.508)
          (fill (type none))
        )
        (circle (center 2.032 0) (radius 0.508)
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_0_1"
        (arc (start 1.524 1.27) (mid 0 1.778) (end -1.524 1.27)
          (fill (type none))
        )
      )
      (symbol "Jumper_2_Open_1_1"
        (pin passive line (at -5.08 0 0) (length 2.54)
          (name "A")
          (number "1")
        )
        (pin passive line (at 5.08 0 180) (length 2.54)
          (name "B")
          (number "2")
        )
      )
    )
    (symbol "Logic_Programmable:PAL20L8" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -8.89 21.59 0))
      (property "Value" "PAL20L8" (id 1) (at 1.27 21.59 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "PAL PLD 20L8" (id 4) (at 0 0 0))
      (property "ki_description" "Programmable Logic Array, DIP-24" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP* PDIP*" (id 6) (at 0 0 0))
      (symbol "PAL20L8_0_0"
        (pin power_in line (at 0 -20.32 90) (length 3.81)
          (name "GND")
          (number "12")
        )
        (pin power_in line (at 0 22.86 270) (length 3.81)
          (name "VCC")
          (number "24")
        )
      )
      (symbol "PAL20L8_0_1"
        (rectangle (start -8.89 19.05) (end 7.62 -16.51)
          (fill (type background))
        )
      )
      (symbol "PAL20L8_1_1"
        (pin input line (at -12.7 17.78 0) (length 3.81)
          (name "I1")
          (number "1")
        )
        (pin input line (at -12.7 -5.08 0) (length 3.81)
          (name "I10")
          (number "10")
        )
        (pin input line (at -12.7 -7.62 0) (length 3.81)
          (name "I11")
          (number "11")
        )
        (pin input line (at -12.7 -10.16 0) (length 3.81)
          (name "I13")
          (number "13")
        )
        (pin input line (at -12.7 -12.7 0) (length 3.81)
          (name "I14")
          (number "14")
        )
        (pin tri_state inverted (at 12.7 0 180) (length 5.08)
          (name "IO15")
          (number "15")
        )
        (pin tri_state inverted (at 12.7 2.54 180) (length 5.08)
          (name "IO16")
          (number "16")
        )
        (pin tri_state inverted (at 12.7 5.08 180) (length 5.08)
          (name "IO17")
          (number "17")
        )
        (pin tri_state inverted (at 12.7 7.62 180) (length 5.08)
          (name "IO18")
          (number "18")
        )
        (pin tri_state inverted (at 12.7 10.16 180) (length 5.08)
          (name "IO19")
          (number "19")
        )
        (pin input line (at -12.7 15.24 0) (length 3.81)
          (name "I2")
          (number "2")
        )
        (pin tri_state inverted (at 12.7 12.7 180) (length 5.08)
          (name "I020")
          (number "20")
        )
        (pin tri_state inverted (at 12.7 15.24 180) (length 5.08)
          (name "IO21")
          (number "21")
        )
        (pin tri_state inverted (at 12.7 17.78 180) (length 5.08)
          (name "IO22")
          (number "22")
        )
        (pin input line (at -12.7 -15.24 0) (length 3.81)
          (name "I23")
          (number "23")
        )
        (pin input line (at -12.7 12.7 0) (length 3.81)
          (name "I3")
          (number "3")
        )
        (pin input line (at -12.7 10.16 0) (length 3.81)
          (name "I4")
          (number "4")
        )
        (pin input line (at -12.7 7.62 0) (length 3.81)
          (name "I5")
          (number "5")
        )
        (pin input line (at -12.7 5.08 0) (length 3.81)
          (name "I6")
          (number "6")
        )
        (pin input line (at -12.7 2.54 0) (length 3.81)
          (name "I7")
          (number "7")
        )
        (pin input line (at -12.7 0 0) (length 3.81)
          (name "I8")
          (number "8")
        )
        (pin input line (at -12.7 -2.54 0) (length 3.81)
          (name "I9")
          (number "9")
        )
      )
    )
    (symbol "Oscillator:SG-8002CA" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "X" (id 0) (at -5.08 6.35 0))
      (property "Value" "SG-8002CA" (id 1) (at 1.27 -6.35 0))
      (property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CA-4Pin_7.0x5.0mm" (id 2) (at 17.78 -8.89 0))
      (property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC" (id 3) (at -2.54 0 0))
      (property "ki_keywords" "Crystal Clock Oscillator" (id 4) (at 0 0 0))
      (property "ki_description" "CMOS Clock Oscillator 1 to 125 MHz" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "Oscillator*SMD*SeikoEpson*SG8002CA*7.0x5.0mm*" (id 6) (at 0 0 0))
      (symbol "SG-8002CA_0_1"
        (rectangle (start -5.08 5.08) (end 5.08 -5.08)
          (fill (type background))
        )
        (polyline
          (pts
            (xy -1.27 -0.762)
            (xy -1.016 -0.762)
            (xy -1.016 0.762)
            (xy -0.508 0.762)
            (xy -0.508 -0.762)
            (xy 0 -0.762)
            (xy 0 0.762)
            (xy 0.508 0.762)
            (xy 0.508 -0.762)
            (xy 0.762 -0.762)
          )
          (fill (type none))
        )
      )
      (symbol "SG-8002CA_1_1"
        (pin input line (at -7.62 0 0) (length 2.54)
          (name "OE")
          (number "1")
        )
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "OUT")
          (number "3")
        )
        (pin power_in line (at 0 7.62 270) (length 2.54)
          (name "Vcc")
          (number "4")
        )
      )
    )
    (symbol "Regulator_Linear:AMS1117CD-1.5" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -3.81 3.175 0))
      (property "Value" "AMS1117CD-1.5" (id 1) (at 0 3.175 0))
      (property "Footprint" "Package_TO_SOT_SMD:TO-252-3_TabPin2" (id 2) (at 0 5.08 0))
      (property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf" (id 3) (at 2.54 -6.35 0))
      (property "ki_keywords" "linear regulator ldo fixed positive" (id 4) (at 0 0 0))
      (property "ki_description" "1A Low Dropout regulator, positive, 1.5V fixed output, TO-252" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "TO?252*TabPin2*" (id 6) (at 0 0 0))
      (symbol "AMS1117CD-1.5_0_1"
        (rectangle (start -5.08 -5.08) (end 5.08 1.905)
          (fill (type background))
        )
      )
      (symbol "AMS1117CD-1.5_1_1"
        (pin power_in line (at 0 -7.62 90) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin power_out line (at 7.62 0 180) (length 2.54)
          (name "VO")
          (number "2")
        )
        (pin power_in line (at -7.62 0 0) (length 2.54)
          (name "VI")
          (number "3")
        )
      )
    )
    (symbol "cbus_288m-rescue:CBUS_EDGE_CON-Audio" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "J" (id 0) (at 0 -2.54 0))
      (property "Value" "CBUS_EDGE_CON-Audio" (id 1) (at 0 2.54 0))
      (property "Footprint" "MODULE" (id 2) (at 0 0 0))
      (property "Datasheet" "DOCUMENTATION" (id 3) (at 0 0 0))
      (symbol "CBUS_EDGE_CON-Audio_1_0"
        (rectangle (start -11.43 -67.31) (end 11.43 67.31)
          (fill (type background))
        )
      )
      (symbol "CBUS_EDGE_CON-Audio_1_1"
        (pin unspecified line (at -19.05 62.23 0) (length 7.62)
          (name "A1")
          (number "1")
        )
        (pin unspecified line (at -19.05 39.37 0) (length 7.62)
          (name "A10")
          (number "10")
        )
        (pin unspecified line (at 19.05 62.23 180) (length 7.62)
          (name "B50")
          (number "100")
        )
        (pin unspecified line (at -19.05 36.83 0) (length 7.62)
          (name "A11")
          (number "11")
        )
        (pin unspecified line (at -19.05 34.29 0) (length 7.62)
          (name "A12")
          (number "12")
        )
        (pin unspecified line (at -19.05 31.75 0) (length 7.62)
          (name "A13")
          (number "13")
        )
        (pin unspecified line (at -19.05 29.21 0) (length 7.62)
          (name "A14")
          (number "14")
        )
        (pin unspecified line (at -19.05 26.67 0) (length 7.62)
          (name "A15")
          (number "15")
        )
        (pin unspecified line (at -19.05 24.13 0) (length 7.62)
          (name "A16")
          (number "16")
        )
        (pin unspecified line (at -19.05 21.59 0) (length 7.62)
          (name "A17")
          (number "17")
        )
        (pin unspecified line (at -19.05 19.05 0) (length 7.62)
          (name "A18")
          (number "18")
        )
        (pin unspecified line (at -19.05 16.51 0) (length 7.62)
          (name "A19")
          (number "19")
        )
        (pin unspecified line (at -19.05 59.69 0) (length 7.62)
          (name "A2")
          (number "2")
        )
        (pin unspecified line (at -19.05 13.97 0) (length 7.62)
          (name "A20")
          (number "20")
        )
        (pin unspecified line (at -19.05 11.43 0) (length 7.62)
          (name "A21")
          (number "21")
        )
        (pin unspecified line (at -19.05 8.89 0) (length 7.62)
          (name "A22")
          (number "22")
        )
        (pin unspecified line (at -19.05 6.35 0) (length 7.62)
          (name "A23")
          (number "23")
        )
        (pin unspecified line (at -19.05 3.81 0) (length 7.62)
          (name "A24")
          (number "24")
        )
        (pin unspecified line (at -19.05 1.27 0) (length 7.62)
          (name "A25")
          (number "25")
        )
        (pin unspecified line (at -19.05 -1.27 0) (length 7.62)
          (name "A26")
          (number "26")
        )
        (pin unspecified line (at -19.05 -3.81 0) (length 7.62)
          (name "A27")
          (number "27")
        )
        (pin unspecified line (at -19.05 -6.35 0) (length 7.62)
          (name "A28")
          (number "28")
        )
        (pin unspecified line (at -19.05 -8.89 0) (length 7.62)
          (name "A29")
          (number "29")
        )
        (pin unspecified line (at -19.05 57.15 0) (length 7.62)
          (name "A3")
          (number "3")
        )
        (pin unspecified line (at -19.05 -11.43 0) (length 7.62)
          (name "A30")
          (number "30")
        )
        (pin unspecified line (at -19.05 -13.97 0) (length 7.62)
          (name "A31")
          (number "31")
        )
        (pin unspecified line (at -19.05 -16.51 0) (length 7.62)
          (name "A32")
          (number "32")
        )
        (pin unspecified line (at -19.05 -19.05 0) (length 7.62)
          (name "A33")
          (number "33")
        )
        (pin unspecified line (at -19.05 -21.59 0) (length 7.62)
          (name "A34")
          (number "34")
        )
        (pin unspecified line (at -19.05 -24.13 0) (length 7.62)
          (name "A35")
          (number "35")
        )
        (pin unspecified line (at -19.05 -26.67 0) (length 7.62)
          (name "A36")
          (number "36")
        )
        (pin unspecified line (at -19.05 -29.21 0) (length 7.62)
          (name "A37")
          (number "37")
        )
        (pin unspecified line (at -19.05 -31.75 0) (length 7.62)
          (name "A38")
          (number "38")
        )
        (pin unspecified line (at -19.05 -34.29 0) (length 7.62)
          (name "A39")
          (number "39")
        )
        (pin unspecified line (at -19.05 54.61 0) (length 7.62)
          (name "A4")
          (number "4")
        )
        (pin unspecified line (at -19.05 -36.83 0) (length 7.62)
          (name "A40")
          (number "40")
        )
        (pin unspecified line (at -19.05 -39.37 0) (length 7.62)
          (name "A41")
          (number "41")
        )
        (pin unspecified line (at -19.05 -41.91 0) (length 7.62)
          (name "A42")
          (number "42")
        )
        (pin unspecified line (at -19.05 -44.45 0) (length 7.62)
          (name "A43")
          (number "43")
        )
        (pin unspecified line (at -19.05 -46.99 0) (length 7.62)
          (name "A44")
          (number "44")
        )
        (pin unspecified line (at -19.05 -49.53 0) (length 7.62)
          (name "A45")
          (number "45")
        )
        (pin unspecified line (at -19.05 -52.07 0) (length 7.62)
          (name "A46")
          (number "46")
        )
        (pin unspecified line (at -19.05 -54.61 0) (length 7.62)
          (name "A47")
          (number "47")
        )
        (pin unspecified line (at -19.05 -57.15 0) (length 7.62)
          (name "A48")
          (number "48")
        )
        (pin unspecified line (at -19.05 -59.69 0) (length 7.62)
          (name "A49")
          (number "49")
        )
        (pin unspecified line (at -19.05 52.07 0) (length 7.62)
          (name "A5")
          (number "5")
        )
        (pin unspecified line (at -19.05 -62.23 0) (length 7.62)
          (name "A50")
          (number "50")
        )
        (pin unspecified line (at 19.05 -62.23 180) (length 7.62)
          (name "B1")
          (number "51")
        )
        (pin unspecified line (at 19.05 -59.69 180) (length 7.62)
          (name "B2")
          (number "52")
        )
        (pin unspecified line (at 19.05 -57.15 180) (length 7.62)
          (name "B3")
          (number "53")
        )
        (pin unspecified line (at 19.05 -54.61 180) (length 7.62)
          (name "B4")
          (number "54")
        )
        (pin unspecified line (at 19.05 -52.07 180) (length 7.62)
          (name "B5")
          (number "55")
        )
        (pin unspecified line (at 19.05 -49.53 180) (length 7.62)
          (name "B6")
          (number "56")
        )
        (pin unspecified line (at 19.05 -46.99 180) (length 7.62)
          (name "B7")
          (number "57")
        )
        (pin unspecified line (at 19.05 -44.45 180) (length 7.62)
          (name "B8")
          (number "58")
        )
        (pin unspecified line (at 19.05 -41.91 180) (length 7.62)
          (name "B9")
          (number "59")
        )
        (pin unspecified line (at -19.05 49.53 0) (length 7.62)
          (name "A6")
          (number "6")
        )
        (pin unspecified line (at 19.05 -39.37 180) (length 7.62)
          (name "B10")
          (number "60")
        )
        (pin unspecified line (at 19.05 -36.83 180) (length 7.62)
          (name "B11")
          (number "61")
        )
        (pin unspecified line (at 19.05 -34.29 180) (length 7.62)
          (name "B12")
          (number "62")
        )
        (pin unspecified line (at 19.05 -31.75 180) (length 7.62)
          (name "B13")
          (number "63")
        )
        (pin unspecified line (at 19.05 -29.21 180) (length 7.62)
          (name "B14")
          (number "64")
        )
        (pin unspecified line (at 19.05 -26.67 180) (length 7.62)
          (name "B15")
          (number "65")
        )
        (pin unspecified line (at 19.05 -24.13 180) (length 7.62)
          (name "B16")
          (number "66")
        )
        (pin unspecified line (at 19.05 -21.59 180) (length 7.62)
          (name "B17")
          (number "67")
        )
        (pin unspecified line (at 19.05 -19.05 180) (length 7.62)
          (name "B18")
          (number "68")
        )
        (pin unspecified line (at 19.05 -16.51 180) (length 7.62)
          (name "B19")
          (number "69")
        )
        (pin unspecified line (at -19.05 46.99 0) (length 7.62)
          (name "A7")
          (number "7")
        )
        (pin unspecified line (at 19.05 -13.97 180) (length 7.62)
          (name "B20")
          (number "70")
        )
        (pin unspecified line (at 19.05 -11.43 180) (length 7.62)
          (name "B21")
          (number "71")
        )
        (pin unspecified line (at 19.05 -8.89 180) (length 7.62)
          (name "B22")
          (number "72")
        )
        (pin unspecified line (at 19.05 -6.35 180) (length 7.62)
          (name "B23")
          (number "73")
        )
        (pin unspecified line (at 19.05 -3.81 180) (length 7.62)
          (name "B24")
          (number "74")
        )
        (pin unspecified line (at 19.05 -1.27 180) (length 7.62)
          (name "B25")
          (number "75")
        )
        (pin unspecified line (at 19.05 1.27 180) (length 7.62)
          (name "B26")
          (number "76")
        )
        (pin unspecified line (at 19.05 3.81 180) (length 7.62)
          (name "B27")
          (number "77")
        )
        (pin unspecified line (at 19.05 6.35 180) (length 7.62)
          (name "B28")
          (number "78")
        )
        (pin unspecified line (at 19.05 8.89 180) (length 7.62)
          (name "B29")
          (number "79")
        )
        (pin unspecified line (at -19.05 44.45 0) (length 7.62)
          (name "A8")
          (number "8")
        )
        (pin unspecified line (at 19.05 11.43 180) (length 7.62)
          (name "B30")
          (number "80")
        )
        (pin unspecified line (at 19.05 13.97 180) (length 7.62)
          (name "B31")
          (number "81")
        )
        (pin unspecified line (at 19.05 16.51 180) (length 7.62)
          (name "B32")
          (number "82")
        )
        (pin unspecified line (at 19.05 19.05 180) (length 7.62)
          (name "B33")
          (number "83")
        )
        (pin unspecified line (at 19.05 21.59 180) (length 7.62)
          (name "B34")
          (number "84")
        )
        (pin unspecified line (at 19.05 24.13 180) (length 7.62)
          (name "B35")
          (number "85")
        )
        (pin unspecified line (at 19.05 26.67 180) (length 7.62)
          (name "B36")
          (number "86")
        )
        (pin unspecified line (at 19.05 29.21 180) (length 7.62)
          (name "B37")
          (number "87")
        )
        (pin unspecified line (at 19.05 31.75 180) (length 7.62)
          (name "B38")
          (number "88")
        )
        (pin unspecified line (at 19.05 34.29 180) (length 7.62)
          (name "B39")
          (number "89")
        )
        (pin unspecified line (at -19.05 41.91 0) (length 7.62)
          (name "A9")
          (number "9")
        )
        (pin unspecified line (at 19.05 36.83 180) (length 7.62)
          (name "B40")
          (number "90")
        )
        (pin unspecified line (at 19.05 39.37 180) (length 7.62)
          (name "B41")
          (number "91")
        )
        (pin unspecified line (at 19.05 41.91 180) (length 7.62)
          (name "B42")
          (number "92")
        )
        (pin unspecified line (at 19.05 44.45 180) (length 7.62)
          (name "B43")
          (number "93")
        )
        (pin unspecified line (at 19.05 46.99 180) (length 7.62)
          (name "B44")
          (number "94")
        )
        (pin unspecified line (at 19.05 49.53 180) (length 7.62)
          (name "B45")
          (number "95")
        )
        (pin unspecified line (at 19.05 52.07 180) (length 7.62)
          (name "B46")
          (number "96")
        )
        (pin unspecified line (at 19.05 54.61 180) (length 7.62)
          (name "B47")
          (number "97")
        )
        (pin unspecified line (at 19.05 57.15 180) (length 7.62)
          (name "B48")
          (number "98")
        )
        (pin unspecified line (at 19.05 59.69 180) (length 7.62)
          (name "B49")
          (number "99")
        )
      )
    )
    (symbol "cbus_288m-rescue:YMF-288M-Audio" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 11.43 0 0))
      (property "Value" "YMF-288M-Audio" (id 1) (at 0 0 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (symbol "YMF-288M-Audio_0_1"
        (rectangle (start -5.08 -2.54) (end 12.7 -40.64)
          (fill (type background))
        )
      )
      (symbol "YMF-288M-Audio_1_1"
        (pin passive line (at -7.62 -5.08 0) (length 2.54)
          (name "VSS")
          (number "1")
        )
        (pin no_connect line (at -7.62 -27.94 0) (length 2.54)
          (name "NC")
          (number "10")
        )
        (pin input line (at -7.62 -30.48 0) (length 2.54)
          (name "/IC")
          (number "11")
        )
        (pin input line (at -7.62 -33.02 0) (length 2.54)
          (name "5/3.3V")
          (number "12")
        )
        (pin no_connect line (at -7.62 -35.56 0) (length 2.54)
          (name "NC")
          (number "13")
        )
        (pin passive line (at -7.62 -38.1 0) (length 2.54)
          (name "VSS")
          (number "14")
        )
        (pin output line (at 15.24 -38.1 180) (length 2.54)
          (name "/IRQ")
          (number "15")
        )
        (pin passive line (at 15.24 -35.56 180) (length 2.54)
          (name "VSS")
          (number "16")
        )
        (pin input line (at 15.24 -33.02 180) (length 2.54)
          (name "/CS")
          (number "17")
        )
        (pin input line (at 15.24 -30.48 180) (length 2.54)
          (name "/WR")
          (number "18")
        )
        (pin input line (at 15.24 -27.94 180) (length 2.54)
          (name "/RD")
          (number "19")
        )
        (pin bidirectional line (at -7.62 -7.62 0) (length 2.54)
          (name "D0")
          (number "2")
        )
        (pin input line (at 15.24 -25.4 180) (length 2.54)
          (name "A0")
          (number "20")
        )
        (pin input line (at 15.24 -22.86 180) (length 2.54)
          (name "A1")
          (number "21")
        )
        (pin power_in line (at 15.24 -20.32 180) (length 2.54)
          (name "VCC")
          (number "22")
        )
        (pin output line (at 15.24 -17.78 180) (length 2.54)
          (name "BCO")
          (number "23")
        )
        (pin output line (at 15.24 -15.24 180) (length 2.54)
          (name "SO")
          (number "24")
        )
        (pin output line (at 15.24 -12.7 180) (length 2.54)
          (name "WCO")
          (number "25")
        )
        (pin output line (at 15.24 -10.16 180) (length 2.54)
          (name "LRO")
          (number "26")
        )
        (pin power_in line (at 15.24 -7.62 180) (length 2.54)
          (name "VCC")
          (number "27")
        )
        (pin input line (at 15.24 -5.08 180) (length 2.54)
          (name "MCLK")
          (number "28")
        )
        (pin bidirectional line (at -7.62 -10.16 0) (length 2.54)
          (name "D1")
          (number "3")
        )
        (pin bidirectional line (at -7.62 -12.7 0) (length 2.54)
          (name "D2")
          (number "4")
        )
        (pin bidirectional line (at -7.62 -15.24 0) (length 2.54)
          (name "D3")
          (number "5")
        )
        (pin bidirectional line (at -7.62 -17.78 0) (length 2.54)
          (name "D4")
          (number "6")
        )
        (pin bidirectional line (at -7.62 -20.32 0) (length 2.54)
          (name "D5")
          (number "7")
        )
        (pin bidirectional line (at -7.62 -22.86 0) (length 2.54)
          (name "D6")
          (number "8")
        )
        (pin bidirectional line (at -7.62 -25.4 0) (length 2.54)
          (name "D7")
          (number "9")
        )
      )
    )
    (symbol "cbus_288m-rescue:uPD6379-Analog_DAC" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 8.89 0 0))
      (property "Value" "uPD6379-Analog_DAC" (id 1) (at -5.08 0 0))
      (property "Footprint" "" (id 2) (at 8.89 0 0))
      (property "Datasheet" "" (id 3) (at 8.89 0 0))
      (symbol "uPD6379-Analog_DAC_0_0"
        (rectangle (start -8.89 -1.27) (end 10.16 -13.97)
          (fill (type background))
        )
      )
      (symbol "uPD6379-Analog_DAC_1_1"
        (pin input line (at -11.43 -3.81 0) (length 2.54)
          (name "LRCK")
          (number "1")
        )
        (pin input line (at -11.43 -6.35 0) (length 2.54)
          (name "SI")
          (number "2")
        )
        (pin input line (at -11.43 -8.89 0) (length 2.54)
          (name "CLK")
          (number "3")
        )
        (pin power_in line (at -11.43 -11.43 0) (length 2.54)
          (name "VDD")
          (number "4")
        )
        (pin output line (at 12.7 -11.43 180) (length 2.54)
          (name "ROUT")
          (number "5")
        )
        (pin input line (at 12.7 -8.89 180) (length 2.54)
          (name "REF")
          (number "6")
        )
        (pin passive line (at 12.7 -6.35 180) (length 2.54)
          (name "GND")
          (number "7")
        )
        (pin output line (at 12.7 -3.81 180) (length 2.54)
          (name "LOUT")
          (number "8")
        )
      )
    )
    (symbol "power:+12VA" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+12VA" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+12VA\"" (id 5) (at 0 0 0))
      (symbol "+12VA_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+12VA_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+12VA")
          (number "1")
        )
      )
    )
    (symbol "power:+5VA" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5VA" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5VA\"" (id 5) (at 0 0 0))
      (symbol "+5VA_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5VA_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5VA")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
    (symbol "power:GNDA" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GNDA" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GNDA\" , analog ground" (id 5) (at 0 0 0))
      (symbol "GNDA_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GNDA_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GNDA")
          (number "1")
        )
      )
    )
    (symbol "power:VCC" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "VCC" (id 1) (at 0 3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "power-flag" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"VCC\"" (id 5) (at 0 0 0))
      (symbol "VCC_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "VCC_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "VCC")
          (number "1")
        )
      )
    )
  )
  (junction (at 176.53 22.86) (diameter 1.016) (color 0 0 0 0))
  (junction (at 127 152.4) (diameter 1.016) (color 0 0 0 0))
  (junction (at 27.94 176.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 248.92 49.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 105.41 171.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 157.48 121.92) (diameter 1.016) (color 0 0 0 0))
  (junction (at 127 124.46) (diameter 1.016) (color 0 0 0 0))
  (junction (at 147.32 186.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 57.15 184.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 130.81 97.79) (diameter 1.016) (color 0 0 0 0))
  (junction (at 127 148.59) (diameter 1.016) (color 0 0 0 0))
  (junction (at 57.15 176.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 146.05 111.76) (diameter 1.016) (color 0 0 0 0))
  (junction (at 19.05 184.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 135.89 186.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 114.3 186.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 238.76 57.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 130.81 90.17) (diameter 1.016) (color 0 0 0 0))
  (junction (at 222.25 49.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 130.81 95.25) (diameter 1.016) (color 0 0 0 0))
  (junction (at 105.41 186.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 222.25 57.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 114.3 171.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 157.48 152.4) (diameter 1.016) (color 0 0 0 0))
  (junction (at 124.46 171.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 195.58 20.32) (diameter 1.016) (color 0 0 0 0))
  (junction (at 177.8 144.78) (diameter 1.016) (color 0 0 0 0))
  (junction (at 251.46 97.79) (diameter 1.016) (color 0 0 0 0))
  (junction (at 157.48 128.27) (diameter 1.016) (color 0 0 0 0))
  (junction (at 96.52 171.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 144.78) (diameter 1.016) (color 0 0 0 0))
  (junction (at 147.32 171.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 109.22 71.12) (diameter 1.016) (color 0 0 0 0))
  (junction (at 82.55 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 248.92 57.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 25.4 149.86) (diameter 1.016) (color 0 0 0 0))
  (junction (at 227.33 142.24) (diameter 1.016) (color 0 0 0 0))
  (junction (at 130.81 87.63) (diameter 1.016) (color 0 0 0 0))
  (junction (at 27.94 184.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 110.49 66.04) (diameter 0) (color 0 0 0 0))
  (junction (at 130.81 100.33) (diameter 1.016) (color 0 0 0 0))
  (junction (at 109.22 107.95) (diameter 1.016) (color 0 0 0 0))
  (junction (at 130.81 85.09) (diameter 1.016) (color 0 0 0 0))
  (junction (at 127 128.27) (diameter 1.016) (color 0 0 0 0))
  (junction (at 66.04 176.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 19.05 176.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 48.26 176.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 66.04 184.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 130.81 92.71) (diameter 1.016) (color 0 0 0 0))
  (junction (at 96.52 186.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 39.37 176.53) (diameter 1.016) (color 0 0 0 0))
  (junction (at 48.26 184.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 124.46 186.69) (diameter 1.016) (color 0 0 0 0))
  (junction (at 213.36 123.19) (diameter 1.016) (color 0 0 0 0))
  (junction (at 157.48 146.05) (diameter 1.016) (color 0 0 0 0))
  (junction (at 123.19 45.72) (diameter 0) (color 0 0 0 0))
  (junction (at 193.04 144.78) (diameter 1.016) (color 0 0 0 0))
  (junction (at 135.89 171.45) (diameter 1.016) (color 0 0 0 0))
  (junction (at 39.37 184.15) (diameter 1.016) (color 0 0 0 0))
  (junction (at 123.19 66.04) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 66.04) (diameter 1.016) (color 0 0 0 0))
  (junction (at 63.5 25.4) (diameter 1.016) (color 0 0 0 0))
  (junction (at 67.31 96.52) (diameter 1.016) (color 0 0 0 0))
  (no_connect (at 149.86 50.8))
  (no_connect (at 149.86 58.42))
  (no_connect (at 172.72 35.56))
  (no_connect (at 203.2 27.94))
  (wire (pts (xy 128.27 85.09) (xy 130.81 85.09)))
  (wire (pts (xy 243.84 154.94) (xy 243.84 149.86)))
  (wire (pts (xy 255.27 134.62) (xy 262.89 134.62)))
  (wire (pts (xy 171.45 140.97) (xy 190.5 140.97)))
  (wire (pts (xy 105.41 184.15) (xy 105.41 186.69)))
  (wire (pts (xy 124.46 186.69) (xy 135.89 186.69)))
  (wire (pts (xy 195.58 19.05) (xy 195.58 20.32)))
  (wire (pts (xy 238.76 57.15) (xy 248.92 57.15)))
  (wire (pts (xy 248.92 57.15) (xy 251.46 57.15)))
  (wire (pts (xy 21.59 45.72) (xy 25.4 45.72)))
  (wire (pts (xy 92.71 148.59) (xy 90.17 148.59)))
  (wire (pts (xy 123.19 66.04) (xy 149.86 66.04)))
  (wire (pts (xy 63.5 93.98) (xy 67.31 93.98)))
  (wire (pts (xy 67.31 93.98) (xy 67.31 96.52)))
  (wire (pts (xy 82.55 58.42) (xy 97.79 58.42)))
  (wire (pts (xy 128.27 90.17) (xy 130.81 90.17)))
  (wire (pts (xy 173.99 81.28) (xy 180.34 81.28)))
  (wire (pts (xy 246.38 49.53) (xy 248.92 49.53)))
  (wire (pts (xy 248.92 49.53) (xy 251.46 49.53)))
  (wire (pts (xy 201.93 123.19) (xy 205.74 123.19)))
  (wire (pts (xy 143.51 43.18) (xy 149.86 43.18)))
  (wire (pts (xy 172.72 50.8) (xy 180.34 50.8)))
  (wire (pts (xy 212.09 97.79) (xy 219.71 97.79)))
  (wire (pts (xy 172.72 43.18) (xy 180.34 43.18)))
  (wire (pts (xy 111.76 124.46) (xy 127 124.46)))
  (wire (pts (xy 127 124.46) (xy 127 128.27)))
  (wire (pts (xy 17.78 109.22) (xy 25.4 109.22)))
  (wire (pts (xy 251.46 97.79) (xy 255.27 97.79)))
  (wire (pts (xy 128.27 102.87) (xy 130.81 102.87)))
  (wire (pts (xy 139.7 83.82) (xy 148.59 83.82)))
  (wire (pts (xy 21.59 55.88) (xy 25.4 55.88)))
  (wire (pts (xy 193.04 134.62) (xy 193.04 144.78)))
  (wire (pts (xy 128.27 97.79) (xy 130.81 97.79)))
  (wire (pts (xy 71.12 139.7) (xy 63.5 139.7)))
  (wire (pts (xy 182.88 142.24) (xy 204.47 142.24)))
  (wire (pts (xy 236.22 142.24) (xy 236.22 149.86)))
  (wire (pts (xy 69.85 78.74) (xy 63.5 78.74)))
  (wire (pts (xy 130.81 100.33) (xy 130.81 97.79)))
  (wire (pts (xy 129.54 119.38) (xy 127 119.38)))
  (wire (pts (xy 139.7 91.44) (xy 148.59 91.44)))
  (wire (pts (xy 139.7 93.98) (xy 148.59 93.98)))
  (wire (pts (xy 27.94 184.15) (xy 39.37 184.15)))
  (wire (pts (xy 39.37 184.15) (xy 48.26 184.15)))
  (wire (pts (xy 48.26 184.15) (xy 57.15 184.15)))
  (wire (pts (xy 57.15 184.15) (xy 66.04 184.15)))
  (wire (pts (xy 227.33 142.24) (xy 227.33 144.78)))
  (wire (pts (xy 185.42 134.62) (xy 185.42 138.43)))
  (wire (pts (xy 19.05 172.72) (xy 19.05 176.53)))
  (wire (pts (xy 17.78 50.8) (xy 25.4 50.8)))
  (wire (pts (xy 82.55 68.58) (xy 100.33 68.58)))
  (wire (pts (xy 71.12 137.16) (xy 63.5 137.16)))
  (wire (pts (xy 100.33 68.58) (xy 100.33 66.04)))
  (wire (pts (xy 220.98 123.19) (xy 220.98 128.27)))
  (wire (pts (xy 127 148.59) (xy 129.54 148.59)))
  (wire (pts (xy 127 124.46) (xy 129.54 124.46)))
  (wire (pts (xy 236.22 149.86) (xy 226.06 149.86)))
  (wire (pts (xy 264.16 134.62) (xy 264.16 144.78)))
  (wire (pts (xy 266.7 134.62) (xy 264.16 134.62)))
  (wire (pts (xy 144.78 121.92) (xy 148.59 121.92)))
  (wire (pts (xy 212.09 95.25) (xy 219.71 95.25)))
  (wire (pts (xy 233.68 142.24) (xy 227.33 142.24)))
  (wire (pts (xy 243.84 97.79) (xy 251.46 97.79)))
  (wire (pts (xy 157.48 121.92) (xy 157.48 128.27)))
  (wire (pts (xy 176.53 20.32) (xy 195.58 20.32)))
  (wire (pts (xy 96.52 184.15) (xy 96.52 186.69)))
  (wire (pts (xy 96.52 186.69) (xy 105.41 186.69)))
  (wire (pts (xy 105.41 186.69) (xy 114.3 186.69)))
  (wire (pts (xy 114.3 186.69) (xy 124.46 186.69)))
  (wire (pts (xy 213.36 102.87) (xy 213.36 100.33)))
  (wire (pts (xy 119.38 87.63) (xy 123.19 87.63)))
  (wire (pts (xy 90.17 40.64) (xy 97.79 40.64)))
  (wire (pts (xy 227.33 137.16) (xy 227.33 142.24)))
  (wire (pts (xy 27.94 176.53) (xy 19.05 176.53)))
  (wire (pts (xy 157.48 146.05) (xy 160.02 146.05)))
  (wire (pts (xy 212.09 102.87) (xy 213.36 102.87)))
  (wire (pts (xy 90.17 30.48) (xy 97.79 30.48)))
  (wire (pts (xy 176.53 20.32) (xy 176.53 22.86)))
  (wire (pts (xy 176.53 22.86) (xy 176.53 30.48)))
  (wire (pts (xy 219.71 102.87) (xy 218.44 102.87)))
  (wire (pts (xy 127 128.27) (xy 127 133.35)))
  (wire (pts (xy 90.17 53.34) (xy 97.79 53.34)))
  (wire (pts (xy 17.78 101.6) (xy 25.4 101.6)))
  (wire (pts (xy 119.38 102.87) (xy 123.19 102.87)))
  (wire (pts (xy 139.7 88.9) (xy 148.59 88.9)))
  (wire (pts (xy 156.21 121.92) (xy 157.48 121.92)))
  (wire (pts (xy 143.51 33.02) (xy 149.86 33.02)))
  (wire (pts (xy 157.48 133.35) (xy 140.97 133.35)))
  (wire (pts (xy 135.89 53.34) (xy 132.08 53.34)))
  (wire (pts (xy 128.27 171.45) (xy 124.46 171.45)))
  (wire (pts (xy 135.89 171.45) (xy 147.32 171.45)))
  (wire (pts (xy 105.41 171.45) (xy 105.41 176.53)))
  (wire (pts (xy 71.12 142.24) (xy 63.5 142.24)))
  (wire (pts (xy 201.93 123.19) (xy 201.93 138.43)))
  (wire (pts (xy 90.17 43.18) (xy 97.79 43.18)))
  (wire (pts (xy 213.36 100.33) (xy 219.71 100.33)))
  (wire (pts (xy 123.19 33.02) (xy 129.54 33.02)))
  (wire (pts (xy 90.17 33.02) (xy 97.79 33.02)))
  (wire (pts (xy 104.14 148.59) (xy 100.33 148.59)))
  (wire (pts (xy 233.68 121.92) (xy 233.68 127)))
  (wire (pts (xy 90.17 35.56) (xy 97.79 35.56)))
  (wire (pts (xy 228.6 137.16) (xy 227.33 137.16)))
  (wire (pts (xy 127 148.59) (xy 127 152.4)))
  (wire (pts (xy 130.81 102.87) (xy 130.81 100.33)))
  (wire (pts (xy 119.38 85.09) (xy 123.19 85.09)))
  (wire (pts (xy 222.25 49.53) (xy 231.14 49.53)))
  (wire (pts (xy 130.81 85.09) (xy 133.35 85.09)))
  (wire (pts (xy 227.33 144.78) (xy 264.16 144.78)))
  (wire (pts (xy 173.99 93.98) (xy 180.34 93.98)))
  (wire (pts (xy 173.99 88.9) (xy 180.34 88.9)))
  (wire (pts (xy 21.59 33.02) (xy 25.4 33.02)))
  (wire (pts (xy 123.19 30.48) (xy 129.54 30.48)))
  (wire (pts (xy 123.19 35.56) (xy 129.54 35.56)))
  (wire (pts (xy 16.51 137.16) (xy 25.4 137.16)))
  (wire (pts (xy 90.17 60.96) (xy 97.79 60.96)))
  (wire (pts (xy 172.72 55.88) (xy 180.34 55.88)))
  (wire (pts (xy 243.84 100.33) (xy 246.38 100.33)))
  (wire (pts (xy 92.71 124.46) (xy 90.17 124.46)))
  (wire (pts (xy 139.7 96.52) (xy 148.59 96.52)))
  (wire (pts (xy 176.53 30.48) (xy 172.72 30.48)))
  (wire (pts (xy 139.7 86.36) (xy 148.59 86.36)))
  (wire (pts (xy 71.12 129.54) (xy 63.5 129.54)))
  (wire (pts (xy 171.45 146.05) (xy 171.45 140.97)))
  (wire (pts (xy 66.04 184.15) (xy 74.93 184.15)))
  (wire (pts (xy 173.99 83.82) (xy 180.34 83.82)))
  (wire (pts (xy 146.05 104.14) (xy 146.05 111.76)))
  (wire (pts (xy 114.3 171.45) (xy 114.3 176.53)))
  (wire (pts (xy 199.39 99.06) (xy 207.01 99.06)))
  (wire (pts (xy 119.38 90.17) (xy 123.19 90.17)))
  (wire (pts (xy 142.24 152.4) (xy 127 152.4)))
  (wire (pts (xy 71.12 121.92) (xy 63.5 121.92)))
  (wire (pts (xy 63.5 124.46) (xy 69.85 124.46)))
  (wire (pts (xy 17.78 25.4) (xy 25.4 25.4)))
  (wire (pts (xy 63.5 27.94) (xy 63.5 25.4)))
  (wire (pts (xy 25.4 147.32) (xy 25.4 149.86)))
  (wire (pts (xy 147.32 171.45) (xy 158.75 171.45)))
  (wire (pts (xy 128.27 87.63) (xy 130.81 87.63)))
  (wire (pts (xy 147.32 186.69) (xy 147.32 182.88)))
  (wire (pts (xy 80.01 50.8) (xy 80.01 46.99)))
  (wire (pts (xy 109.22 107.95) (xy 140.97 107.95)))
  (wire (pts (xy 140.97 107.95) (xy 140.97 111.76)))
  (wire (pts (xy 140.97 111.76) (xy 146.05 111.76)))
  (wire (pts (xy 243.84 95.25) (xy 257.81 95.25)))
  (wire (pts (xy 143.51 30.48) (xy 149.86 30.48)))
  (wire (pts (xy 149.86 60.96) (xy 149.86 66.04)))
  (wire (pts (xy 243.84 105.41) (xy 257.81 105.41)))
  (wire (pts (xy 90.17 92.71) (xy 99.06 92.71)))
  (wire (pts (xy 139.7 81.28) (xy 148.59 81.28)))
  (wire (pts (xy 127 152.4) (xy 127 157.48)))
  (wire (pts (xy 17.78 129.54) (xy 25.4 129.54)))
  (wire (pts (xy 158.75 171.45) (xy 158.75 175.26)))
  (wire (pts (xy 149.86 152.4) (xy 157.48 152.4)))
  (wire (pts (xy 110.49 66.04) (xy 123.19 66.04)))
  (wire (pts (xy 193.04 144.78) (xy 220.98 144.78)))
  (wire (pts (xy 90.17 45.72) (xy 97.79 45.72)))
  (wire (pts (xy 119.38 100.33) (xy 123.19 100.33)))
  (wire (pts (xy 142.24 128.27) (xy 127 128.27)))
  (wire (pts (xy 17.78 127) (xy 25.4 127)))
  (wire (pts (xy 133.35 80.01) (xy 133.35 78.74)))
  (wire (pts (xy 104.14 124.46) (xy 100.33 124.46)))
  (wire (pts (xy 143.51 40.64) (xy 149.86 40.64)))
  (wire (pts (xy 63.5 99.06) (xy 69.85 99.06)))
  (wire (pts (xy 157.48 128.27) (xy 157.48 133.35)))
  (wire (pts (xy 113.03 143.51) (xy 119.38 143.51)))
  (wire (pts (xy 157.48 146.05) (xy 157.48 152.4)))
  (wire (pts (xy 195.58 35.56) (xy 195.58 66.04)))
  (wire (pts (xy 195.58 66.04) (xy 149.86 66.04)))
  (wire (pts (xy 130.81 87.63) (xy 130.81 85.09)))
  (wire (pts (xy 172.72 33.02) (xy 180.34 33.02)))
  (wire (pts (xy 135.89 182.88) (xy 135.89 186.69)))
  (wire (pts (xy 17.78 76.2) (xy 25.4 76.2)))
  (wire (pts (xy 71.12 132.08) (xy 63.5 132.08)))
  (wire (pts (xy 140.97 53.34) (xy 149.86 53.34)))
  (wire (pts (xy 157.48 152.4) (xy 157.48 157.48)))
  (wire (pts (xy 119.38 92.71) (xy 123.19 92.71)))
  (wire (pts (xy 156.21 146.05) (xy 157.48 146.05)))
  (wire (pts (xy 139.7 101.6) (xy 148.59 101.6)))
  (wire (pts (xy 256.54 57.15) (xy 262.89 57.15)))
  (wire (pts (xy 158.75 182.88) (xy 158.75 186.69)))
  (wire (pts (xy 220.98 135.89) (xy 220.98 144.78)))
  (wire (pts (xy 123.19 38.1) (xy 129.54 38.1)))
  (wire (pts (xy 130.81 92.71) (xy 130.81 90.17)))
  (wire (pts (xy 90.17 27.94) (xy 97.79 27.94)))
  (wire (pts (xy 143.51 45.72) (xy 149.86 45.72)))
  (wire (pts (xy 90.17 87.63) (xy 99.06 87.63)))
  (wire (pts (xy 173.99 78.74) (xy 180.34 78.74)))
  (wire (pts (xy 111.76 148.59) (xy 127 148.59)))
  (wire (pts (xy 204.47 130.81) (xy 204.47 142.24)))
  (wire (pts (xy 69.85 149.86) (xy 63.5 149.86)))
  (wire (pts (xy 213.36 123.19) (xy 220.98 123.19)))
  (wire (pts (xy 238.76 149.86) (xy 238.76 142.24)))
  (wire (pts (xy 172.72 38.1) (xy 180.34 38.1)))
  (wire (pts (xy 133.35 157.48) (xy 127 157.48)))
  (wire (pts (xy 27.94 176.53) (xy 39.37 176.53)))
  (wire (pts (xy 39.37 176.53) (xy 48.26 176.53)))
  (wire (pts (xy 48.26 176.53) (xy 57.15 176.53)))
  (wire (pts (xy 57.15 176.53) (xy 66.04 176.53)))
  (wire (pts (xy 66.04 176.53) (xy 74.93 176.53)))
  (wire (pts (xy 212.09 99.06) (xy 212.09 97.79)))
  (wire (pts (xy 133.35 133.35) (xy 127 133.35)))
  (wire (pts (xy 123.19 45.72) (xy 129.54 45.72)))
  (wire (pts (xy 172.72 60.96) (xy 180.34 60.96)))
  (wire (pts (xy 199.39 102.87) (xy 207.01 102.87)))
  (wire (pts (xy 71.12 127) (xy 63.5 127)))
  (wire (pts (xy 167.64 121.92) (xy 171.45 121.92)))
  (wire (pts (xy 172.72 27.94) (xy 187.96 27.94)))
  (wire (pts (xy 262.89 137.16) (xy 266.7 137.16)))
  (wire (pts (xy 171.45 138.43) (xy 185.42 138.43)))
  (wire (pts (xy 17.78 106.68) (xy 25.4 106.68)))
  (wire (pts (xy 143.51 27.94) (xy 149.86 27.94)))
  (wire (pts (xy 128.27 92.71) (xy 130.81 92.71)))
  (wire (pts (xy 21.59 38.1) (xy 25.4 38.1)))
  (wire (pts (xy 63.5 25.4) (xy 72.39 25.4)))
  (wire (pts (xy 100.33 66.04) (xy 110.49 66.04)))
  (wire (pts (xy 172.72 58.42) (xy 180.34 58.42)))
  (wire (pts (xy 135.89 171.45) (xy 135.89 175.26)))
  (wire (pts (xy 128.27 100.33) (xy 130.81 100.33)))
  (wire (pts (xy 147.32 171.45) (xy 147.32 175.26)))
  (wire (pts (xy 187.96 138.43) (xy 201.93 138.43)))
  (wire (pts (xy 20.32 58.42) (xy 25.4 58.42)))
  (wire (pts (xy 96.52 171.45) (xy 96.52 176.53)))
  (wire (pts (xy 105.41 171.45) (xy 96.52 171.45)))
  (wire (pts (xy 114.3 171.45) (xy 105.41 171.45)))
  (wire (pts (xy 124.46 171.45) (xy 114.3 171.45)))
  (wire (pts (xy 114.3 184.15) (xy 114.3 186.69)))
  (wire (pts (xy 172.72 53.34) (xy 180.34 53.34)))
  (wire (pts (xy 190.5 134.62) (xy 190.5 140.97)))
  (wire (pts (xy 63.5 66.04) (xy 69.85 66.04)))
  (wire (pts (xy 109.22 107.95) (xy 109.22 110.49)))
  (wire (pts (xy 251.46 100.33) (xy 251.46 97.79)))
  (wire (pts (xy 123.19 27.94) (xy 129.54 27.94)))
  (wire (pts (xy 226.06 149.86) (xy 226.06 154.94)))
  (wire (pts (xy 224.79 132.08) (xy 228.6 132.08)))
  (wire (pts (xy 199.39 95.25) (xy 207.01 95.25)))
  (wire (pts (xy 143.51 48.26) (xy 149.86 48.26)))
  (wire (pts (xy 90.17 55.88) (xy 97.79 55.88)))
  (wire (pts (xy 157.48 157.48) (xy 140.97 157.48)))
  (wire (pts (xy 171.45 121.92) (xy 171.45 138.43)))
  (wire (pts (xy 123.19 50.8) (xy 123.19 66.04)))
  (wire (pts (xy 17.78 149.86) (xy 25.4 149.86)))
  (wire (pts (xy 218.44 102.87) (xy 218.44 106.68)))
  (wire (pts (xy 21.59 43.18) (xy 25.4 43.18)))
  (wire (pts (xy 130.81 97.79) (xy 130.81 95.25)))
  (wire (pts (xy 158.75 186.69) (xy 147.32 186.69)))
  (wire (pts (xy 243.84 149.86) (xy 238.76 149.86)))
  (wire (pts (xy 63.5 48.26) (xy 69.85 48.26)))
  (wire (pts (xy 119.38 97.79) (xy 123.19 97.79)))
  (wire (pts (xy 110.49 22.86) (xy 176.53 22.86)))
  (wire (pts (xy 173.99 86.36) (xy 180.34 86.36)))
  (wire (pts (xy 204.47 130.81) (xy 205.74 130.81)))
  (wire (pts (xy 16.51 139.7) (xy 25.4 139.7)))
  (wire (pts (xy 243.84 102.87) (xy 243.84 105.41)))
  (wire (pts (xy 90.17 100.33) (xy 99.06 100.33)))
  (wire (pts (xy 130.81 95.25) (xy 130.81 92.71)))
  (wire (pts (xy 135.89 186.69) (xy 147.32 186.69)))
  (wire (pts (xy 146.05 111.76) (xy 161.29 111.76)))
  (wire (pts (xy 187.96 134.62) (xy 187.96 138.43)))
  (wire (pts (xy 19.05 184.15) (xy 19.05 187.96)))
  (wire (pts (xy 182.88 134.62) (xy 182.88 142.24)))
  (wire (pts (xy 109.22 71.12) (xy 161.29 71.12)))
  (wire (pts (xy 109.22 80.01) (xy 109.22 71.12)))
  (wire (pts (xy 148.59 104.14) (xy 146.05 104.14)))
  (wire (pts (xy 256.54 49.53) (xy 262.89 49.53)))
  (wire (pts (xy 123.19 40.64) (xy 129.54 40.64)))
  (wire (pts (xy 177.8 129.54) (xy 177.8 144.78)))
  (wire (pts (xy 119.38 95.25) (xy 123.19 95.25)))
  (wire (pts (xy 21.59 53.34) (xy 25.4 53.34)))
  (wire (pts (xy 113.03 119.38) (xy 119.38 119.38)))
  (wire (pts (xy 143.51 35.56) (xy 149.86 35.56)))
  (wire (pts (xy 213.36 130.81) (xy 213.36 123.19)))
  (wire (pts (xy 167.64 146.05) (xy 171.45 146.05)))
  (wire (pts (xy 262.89 134.62) (xy 262.89 137.16)))
  (wire (pts (xy 173.99 91.44) (xy 180.34 91.44)))
  (wire (pts (xy 130.81 90.17) (xy 130.81 87.63)))
  (wire (pts (xy 143.51 38.1) (xy 149.86 38.1)))
  (wire (pts (xy 177.8 144.78) (xy 193.04 144.78)))
  (wire (pts (xy 63.5 96.52) (xy 67.31 96.52)))
  (wire (pts (xy 67.31 96.52) (xy 71.12 96.52)))
  (wire (pts (xy 177.8 144.78) (xy 177.8 149.86)))
  (wire (pts (xy 71.12 134.62) (xy 63.5 134.62)))
  (wire (pts (xy 172.72 45.72) (xy 180.34 45.72)))
  (wire (pts (xy 129.54 143.51) (xy 127 143.51)))
  (wire (pts (xy 80.01 58.42) (xy 82.55 58.42)))
  (wire (pts (xy 173.99 96.52) (xy 180.34 96.52)))
  (wire (pts (xy 128.27 95.25) (xy 130.81 95.25)))
  (wire (pts (xy 90.17 38.1) (xy 97.79 38.1)))
  (wire (pts (xy 144.78 146.05) (xy 148.59 146.05)))
  (wire (pts (xy 139.7 78.74) (xy 148.59 78.74)))
  (wire (pts (xy 90.17 95.25) (xy 99.06 95.25)))
  (wire (pts (xy 27.94 184.15) (xy 19.05 184.15)))
  (wire (pts (xy 172.72 40.64) (xy 180.34 40.64)))
  (wire (pts (xy 82.55 50.8) (xy 97.79 50.8)))
  (wire (pts (xy 157.48 121.92) (xy 160.02 121.92)))
  (wire (pts (xy 82.55 45.72) (xy 82.55 41.91)))
  (wire (pts (xy 222.25 57.15) (xy 238.76 57.15)))
  (wire (pts (xy 21.59 48.26) (xy 25.4 48.26)))
  (wire (pts (xy 123.19 43.18) (xy 129.54 43.18)))
  (wire (pts (xy 63.5 73.66) (xy 69.85 73.66)))
  (wire (pts (xy 21.59 40.64) (xy 25.4 40.64)))
  (wire (pts (xy 90.17 48.26) (xy 97.79 48.26)))
  (wire (pts (xy 172.72 48.26) (xy 180.34 48.26)))
  (wire (pts (xy 21.59 35.56) (xy 25.4 35.56)))
  (wire (pts (xy 149.86 128.27) (xy 157.48 128.27)))
  (wire (pts (xy 243.84 134.62) (xy 247.65 134.62)))
  (wire (pts (xy 226.06 154.94) (xy 228.6 154.94)))
  (wire (pts (xy 80.01 58.42) (xy 80.01 55.88)))
  (text "OPN3 REMASTERED" (at 196.85 85.09 0))
  (text "caution: 6379a is pin-reversed" (at 224.79 111.76 0))
  (text "default 188h, close for 88h" (at 77.47 71.12 0))
  (text "short L2 if amps have problems" (at 240.03 66.04 0))
  (label "DB6" (at 144.78 45.72 0) (fields_autoplaced))
  (label "VREF" (at 152.4 171.45 0) (fields_autoplaced))
  (label "LA" (at 254 95.25 0) (fields_autoplaced))
  (label "A6" (at 24.13 48.26 0) (fields_autoplaced))
  (label "A4" (at 24.13 43.18 0) (fields_autoplaced))
  (label "D1" (at 66.04 139.7 0) (fields_autoplaced))
  (label "DB1" (at 175.26 81.28 0) (fields_autoplaced))
  (label "DB3" (at 144.78 38.1 0) (fields_autoplaced))
  (label "DB4" (at 175.26 88.9 0) (fields_autoplaced))
  (label "D7" (at 66.04 121.92 0) (fields_autoplaced))
  (label "RA" (at 254 105.41 0) (fields_autoplaced))
  (label "RA" (at 90.17 148.59 0) (fields_autoplaced))
  (label "DB7" (at 144.78 48.26 0) (fields_autoplaced))
  (label "D4" (at 66.04 132.08 0) (fields_autoplaced))
  (label "A1" (at 24.13 35.56 0) (fields_autoplaced))
  (label "DSB" (at 93.98 95.25 0) (fields_autoplaced))
  (label "D5" (at 66.04 129.54 0) (fields_autoplaced))
  (label "D3" (at 66.04 134.62 0) (fields_autoplaced))
  (label "D5" (at 143.51 91.44 0) (fields_autoplaced))
  (label "SEL2" (at 124.46 45.72 0) (fields_autoplaced))
  (label "~{CS}" (at 124.46 30.48 0) (fields_autoplaced))
  (label "DSA" (at 93.98 92.71 0) (fields_autoplaced))
  (label "Q" (at 92.71 60.96 0) (fields_autoplaced))
  (label "IORDY" (at 124.46 43.18 0) (fields_autoplaced))
  (label "~{MR}" (at 93.98 87.63 0) (fields_autoplaced))
  (label "~{IOW}" (at 92.71 55.88 0) (fields_autoplaced))
  (label "A7" (at 24.13 53.34 0) (fields_autoplaced))
  (label "DB0" (at 175.26 78.74 0) (fields_autoplaced))
  (label "A8" (at 92.71 43.18 0) (fields_autoplaced))
  (label "D6" (at 66.04 127 0) (fields_autoplaced))
  (label "SO" (at 175.26 38.1 0) (fields_autoplaced))
  (label "D3" (at 143.51 86.36 0) (fields_autoplaced))
  (label "~{IOR}" (at 175.26 50.8 0) (fields_autoplaced))
  (label "~{IOR}" (at 92.71 53.34 0) (fields_autoplaced))
  (label "A4" (at 92.71 33.02 0) (fields_autoplaced))
  (label "D4" (at 143.51 88.9 0) (fields_autoplaced))
  (label "INT5" (at 64.77 78.74 0) (fields_autoplaced))
  (label "A5" (at 24.13 45.72 0) (fields_autoplaced))
  (label "A3" (at 24.13 40.64 0) (fields_autoplaced))
  (label "VREF" (at 114.3 119.38 0) (fields_autoplaced))
  (label "A0" (at 92.71 27.94 0) (fields_autoplaced))
  (label "D1" (at 143.51 81.28 0) (fields_autoplaced))
  (label "DB7" (at 175.26 96.52 0) (fields_autoplaced))
  (label "BCO" (at 175.26 40.64 0) (fields_autoplaced))
  (label "~{MR}" (at 124.46 35.56 0) (fields_autoplaced))
  (label "A9" (at 21.59 58.42 0) (fields_autoplaced))
  (label "~{IOW}" (at 20.32 109.22 0) (fields_autoplaced))
  (label "A2" (at 177.8 45.72 0) (fields_autoplaced))
  (label "DSA" (at 124.46 38.1 0) (fields_autoplaced))
  (label "A8" (at 24.13 55.88 0) (fields_autoplaced))
  (label "~{RST}" (at 144.78 53.34 0) (fields_autoplaced))
  (label "DB1" (at 144.78 33.02 0) (fields_autoplaced))
  (label "Q" (at 130.81 85.09 0) (fields_autoplaced))
  (label "BCO" (at 200.66 102.87 0) (fields_autoplaced))
  (label "~{DIR}" (at 124.46 33.02 0) (fields_autoplaced))
  (label "DSB" (at 124.46 40.64 0) (fields_autoplaced))
  (label "DB3" (at 175.26 86.36 0) (fields_autoplaced))
  (label "D7" (at 143.51 96.52 0) (fields_autoplaced))
  (label "~{DIR}" (at 143.51 101.6 0) (fields_autoplaced))
  (label "DB6" (at 175.26 93.98 0) (fields_autoplaced))
  (label "~{RST}" (at 66.04 66.04 0) (fields_autoplaced))
  (label "A1" (at 177.8 48.26 0) (fields_autoplaced))
  (label "DB5" (at 175.26 91.44 0) (fields_autoplaced))
  (label "A9" (at 92.71 45.72 0) (fields_autoplaced))
  (label "A5" (at 92.71 35.56 0) (fields_autoplaced))
  (label "DB0" (at 144.78 30.48 0) (fields_autoplaced))
  (label "~{EN}" (at 19.05 129.54 0) (fields_autoplaced))
  (label "CLK" (at 93.98 100.33 0) (fields_autoplaced))
  (label "D2" (at 66.04 137.16 0) (fields_autoplaced))
  (label "D0" (at 66.04 142.24 0) (fields_autoplaced))
  (label "DB5" (at 144.78 43.18 0) (fields_autoplaced))
  (label "~{IOR}" (at 20.32 106.68 0) (fields_autoplaced))
  (label "~{CS}" (at 175.26 55.88 0) (fields_autoplaced))
  (label "A3" (at 92.71 30.48 0) (fields_autoplaced))
  (label "SEL1" (at 92.71 58.42 0) (fields_autoplaced))
  (label "LRO" (at 200.66 95.25 0) (fields_autoplaced))
  (label "DB2" (at 175.26 83.82 0) (fields_autoplaced))
  (label "~{IRQ}" (at 175.26 60.96 0) (fields_autoplaced))
  (label "D6" (at 143.51 93.98 0) (fields_autoplaced))
  (label "A6" (at 92.71 38.1 0) (fields_autoplaced))
  (label "A2" (at 24.13 38.1 0) (fields_autoplaced))
  (label "~{IOW}" (at 175.26 53.34 0) (fields_autoplaced))
  (label "D0" (at 143.51 78.74 0) (fields_autoplaced))
  (label "~{EN}" (at 92.71 48.26 0) (fields_autoplaced))
  (label "INT5" (at 124.46 27.94 0) (fields_autoplaced))
  (label "D2" (at 143.51 83.82 0) (fields_autoplaced))
  (label "DB4" (at 144.78 40.64 0) (fields_autoplaced))
  (label "SO" (at 200.66 99.06 0) (fields_autoplaced))
  (label "~{IRQ}" (at 92.71 50.8 0) (fields_autoplaced))
  (label "A0" (at 24.13 33.02 0) (fields_autoplaced))
  (label "DB2" (at 144.78 35.56 0) (fields_autoplaced))
  (label "A7" (at 92.71 40.64 0) (fields_autoplaced))
  (label "LA" (at 90.17 124.46 0) (fields_autoplaced))
  (label "IORDY" (at 19.05 137.16 0) (fields_autoplaced))
  (label "CLK" (at 19.05 139.7 0) (fields_autoplaced))
  (label "VREF" (at 114.3 143.51 0) (fields_autoplaced))
  (label "LRO" (at 175.26 33.02 0) (fields_autoplaced))
  (symbol (lib_id "Device:C") (at 158.75 179.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C3" (id 0) (at 161.671 177.9016 0))
    (property "Value" "0.1UF" (id 1) (at 161.671 180.213 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 159.7152 182.88 0))
    (property "Datasheet" "~" (id 3) (at 158.75 179.07 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VCC") (at 149.86 55.88 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR06" (id 0) (at 153.67 55.88 0))
    (property "Value" "VCC" (id 1) (at 145.4658 55.4482 0))
    (property "Footprint" "" (id 2) (at 149.86 55.88 0))
    (property "Datasheet" "" (id 3) (at 149.86 55.88 0))
    (pin "1")
  )
  (symbol (lib_id "Device:CP1") (at 251.46 134.62 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C7" (id 0) (at 251.46 128.2192 90))
    (property "Value" "220uf" (id 1) (at 251.46 130.5306 90))
    (property "Footprint" "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (id 2) (at 251.46 134.62 0))
    (property "Datasheet" "~" (id 3) (at 251.46 134.62 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VCC") (at 233.68 121.92 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR?" (id 0) (at 233.68 125.73 0))
    (property "Value" "VCC" (id 1) (at 234.1118 117.5258 0))
    (property "Footprint" "" (id 2) (at 233.68 121.92 0))
    (property "Datasheet" "" (id 3) (at 233.68 121.92 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74LS245") (at 161.29 91.44 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U4" (id 0) (at 161.29 66.8994 0))
    (property "Value" "74LS245" (id 1) (at 161.29 69.6745 0))
    (property "Footprint" "Package_SO:SO-20_5.3x12.6mm_P1.27mm" (id 2) (at 161.29 91.44 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS245" (id 3) (at 161.29 91.44 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:C") (at 147.32 179.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C2" (id 0) (at 150.241 177.9016 0))
    (property "Value" "10UF" (id 1) (at 150.241 180.213 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 148.2852 182.88 0))
    (property "Datasheet" "~" (id 3) (at 147.32 179.07 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 133.35 82.55 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R20" (id 0) (at 132.207 78.74 90))
    (property "Value" "10K" (id 1) (at 129.8956 78.74 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 133.35 82.55 0))
    (property "Datasheet" "~" (id 3) (at 133.35 82.55 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 138.43 53.34 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R4" (id 0) (at 138.43 48.133 90))
    (property "Value" "10K" (id 1) (at 138.43 50.4444 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 138.43 53.34 0))
    (property "Datasheet" "~" (id 3) (at 138.43 53.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+12VA") (at 71.12 96.52 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 71.12 100.33 0))
    (property "Value" "+12VA" (id 1) (at 71.12 92.9154 0))
    (property "Footprint" "" (id 2) (at 71.12 96.52 0))
    (property "Datasheet" "" (id 3) (at 71.12 96.52 0))
    (pin "1")
  )
  (symbol (lib_id "power:VCC") (at 132.08 53.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR05" (id 0) (at 132.08 57.15 0))
    (property "Value" "VCC" (id 1) (at 132.5118 48.9458 0))
    (property "Footprint" "" (id 2) (at 132.08 53.34 0))
    (property "Datasheet" "" (id 3) (at 132.08 53.34 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 17.78 101.6 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0110" (id 0) (at 11.43 101.6 0))
    (property "Value" "GND" (id 1) (at 13.3858 101.727 0))
    (property "Footprint" "" (id 2) (at 17.78 101.6 0))
    (property "Datasheet" "" (id 3) (at 17.78 101.6 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_US") (at 152.4 146.05 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R14" (id 0) (at 152.4 140.843 90))
    (property "Value" "10" (id 1) (at 152.4 143.1544 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 152.146 147.066 90))
    (property "Datasheet" "~" (id 3) (at 152.4 146.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5VA") (at 262.89 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0116" (id 0) (at 262.89 53.34 0))
    (property "Value" "+5VA" (id 1) (at 262.89 45.9254 0))
    (property "Footprint" "" (id 2) (at 262.89 49.53 0))
    (property "Datasheet" "" (id 3) (at 262.89 49.53 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 96.52 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C16" (id 0) (at 99.441 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 99.441 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 97.4852 184.15 0))
    (property "Datasheet" "~" (id 3) (at 96.52 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VCC") (at 195.58 19.05 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR02" (id 0) (at 195.58 22.86 0))
    (property "Value" "VCC" (id 1) (at 196.0118 14.6558 0))
    (property "Footprint" "" (id 2) (at 195.58 19.05 0))
    (property "Datasheet" "" (id 3) (at 195.58 19.05 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_US") (at 132.08 171.45 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R5" (id 0) (at 130.9116 169.7228 0))
    (property "Value" "470" (id 1) (at 133.223 169.7228 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 132.334 170.434 90))
    (property "Datasheet" "~" (id 3) (at 132.08 171.45 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 125.73 102.87 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP8" (id 0) (at 123.19 101.2974 0))
    (property "Value" "Jumper_NO_Small" (id 1) (at 125.73 101.2975 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 125.73 102.87 0))
    (property "Datasheet" "~" (id 3) (at 125.73 102.87 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Small") (at 254 49.53 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "L1" (id 0) (at 254 45.1824 90))
    (property "Value" "10UH" (id 1) (at 254 47.9575 90))
    (property "Footprint" "Inductor_SMD:L_1206_3216Metric" (id 2) (at 254 49.53 0))
    (property "Datasheet" "~" (id 3) (at 254 49.53 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VCC") (at 19.05 172.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR013" (id 0) (at 19.05 176.53 0))
    (property "Value" "VCC" (id 1) (at 19.4818 168.3258 0))
    (property "Footprint" "" (id 2) (at 19.05 172.72 0))
    (property "Datasheet" "" (id 3) (at 19.05 172.72 0))
    (pin "1")
  )
  (symbol (lib_id "Device:CP1") (at 222.25 53.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C14" (id 0) (at 225.171 52.1716 0))
    (property "Value" "100UF" (id 1) (at 225.171 54.483 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (id 2) (at 222.25 53.34 0))
    (property "Datasheet" "~" (id 3) (at 222.25 53.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 107.95 124.46 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R10" (id 0) (at 106.7816 122.7328 0))
    (property "Value" "5.6K" (id 1) (at 109.093 122.7328 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 108.204 123.444 90))
    (property "Datasheet" "~" (id 3) (at 107.95 124.46 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 209.55 130.81 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R11" (id 0) (at 209.55 125.603 90))
    (property "Value" "10K" (id 1) (at 209.55 127.9144 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 209.296 131.826 90))
    (property "Datasheet" "~" (id 3) (at 209.55 130.81 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:+5VA") (at 96.52 171.45 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0106" (id 0) (at 96.52 175.26 0))
    (property "Value" "+5VA" (id 1) (at 96.52 167.8454 0))
    (property "Footprint" "" (id 2) (at 96.52 171.45 0))
    (property "Datasheet" "" (id 3) (at 96.52 171.45 0))
    (pin "1")
  )
  (symbol (lib_id "Logic_Programmable:PAL20L8") (at 110.49 45.72 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U3" (id 0) (at 110.49 18.6394 0))
    (property "Value" "GAL20V8" (id 1) (at 110.49 21.4145 0))
    (property "Footprint" "Package_DIP:DIP-24_W7.62mm" (id 2) (at 110.49 45.72 0))
    (property "Datasheet" "" (id 3) (at 110.49 45.72 0))
    (pin "12")
    (pin "24")
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:R_US") (at 123.19 143.51 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R13" (id 0) (at 122.0216 141.7828 0))
    (property "Value" "3.3K" (id 1) (at 124.333 141.7828 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 123.444 142.494 90))
    (property "Datasheet" "~" (id 3) (at 123.19 143.51 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small_US") (at 80.01 53.34 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R19" (id 0) (at 85.217 53.34 90))
    (property "Value" "10K" (id 1) (at 82.9056 53.34 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 80.01 53.34 0))
    (property "Datasheet" "~" (id 3) (at 80.01 53.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP1_Small") (at 248.92 100.33 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C1" (id 0) (at 248.92 103.4288 90))
    (property "Value" "10UF" (id 1) (at 248.92 96.8502 90))
    (property "Footprint" "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A" (id 2) (at 248.92 100.33 0))
    (property "Datasheet" "~" (id 3) (at 248.92 100.33 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP1") (at 27.94 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C13" (id 0) (at 30.861 179.1716 0))
    (property "Value" "100UF" (id 1) (at 30.861 181.483 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (id 2) (at 27.94 180.34 0))
    (property "Datasheet" "~" (id 3) (at 27.94 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 39.37 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C18" (id 0) (at 42.291 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 42.291 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 40.3352 184.15 0))
    (property "Datasheet" "~" (id 3) (at 39.37 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Jumper:Jumper_2_Open") (at 82.55 63.5 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "JP?" (id 0) (at 83.82 62.865 90))
    (property "Value" "NO" (id 1) (at 83.82 65.405 90))
    (property "Footprint" "" (id 2) (at 82.55 63.5 0))
    (property "Datasheet" "~" (id 3) (at 82.55 63.5 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:L_Small") (at 254 57.15 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "L2" (id 0) (at 254 59.1524 90))
    (property "Value" "10UH" (id 1) (at 254 61.9275 90))
    (property "Footprint" "Inductor_SMD:L_1206_3216Metric" (id 2) (at 254 57.15 0))
    (property "Datasheet" "~" (id 3) (at 254 57.15 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP_Small") (at 241.3 154.94 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C11" (id 0) (at 241.3 149.225 90))
    (property "Value" "10UF" (id 1) (at 241.3 151.5364 90))
    (property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (id 2) (at 241.3 154.94 0))
    (property "Datasheet" "~" (id 3) (at 241.3 154.94 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 163.83 146.05 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C8" (id 0) (at 163.83 139.6492 90))
    (property "Value" "10UF" (id 1) (at 163.83 141.9606 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 160.02 147.0152 0))
    (property "Datasheet" "~" (id 3) (at 163.83 146.05 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 125.73 100.33 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP7" (id 0) (at 123.19 98.7574 0))
    (property "Value" "Jumper_NO_Small" (id 1) (at 125.73 98.7575 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 125.73 100.33 0))
    (property "Datasheet" "~" (id 3) (at 125.73 100.33 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 57.15 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C20" (id 0) (at 60.071 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 60.071 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 58.1152 184.15 0))
    (property "Datasheet" "~" (id 3) (at 57.15 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 135.89 179.07 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R6" (id 0) (at 137.6172 177.9016 0))
    (property "Value" "680" (id 1) (at 137.6172 180.213 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 136.906 179.324 90))
    (property "Datasheet" "~" (id 3) (at 135.89 179.07 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 69.85 99.06 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0122" (id 0) (at 76.2 99.06 0))
    (property "Value" "GND" (id 1) (at 74.2442 98.933 0))
    (property "Footprint" "" (id 2) (at 69.85 99.06 0))
    (property "Datasheet" "" (id 3) (at 69.85 99.06 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_US") (at 107.95 148.59 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R15" (id 0) (at 106.7816 146.8628 0))
    (property "Value" "5.6K" (id 1) (at 109.093 146.8628 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 108.204 147.574 90))
    (property "Datasheet" "~" (id 3) (at 107.95 148.59 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "cbus_288m-rescue:YMF-288M-Audio") (at 157.48 22.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U1" (id 0) (at 161.29 21.209 0))
    (property "Value" "YMF-288M" (id 1) (at 161.29 23.5204 0))
    (property "Footprint" "Package_SO:SOIC-28W_7.5x18.7mm_P1.27mm" (id 2) (at 157.48 22.86 0))
    (property "Datasheet" "" (id 3) (at 157.48 22.86 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 125.73 95.25 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP5" (id 0) (at 123.19 93.6774 0))
    (property "Value" "Jumper_NO_Small" (id 1) (at 125.73 93.6775 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 125.73 95.25 0))
    (property "Datasheet" "~" (id 3) (at 125.73 95.25 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Amplifier_Audio:LM386") (at 236.22 134.62 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U7" (id 0) (at 244.9576 133.4516 0))
    (property "Value" "LM386" (id 1) (at 244.9576 135.763 0))
    (property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (id 2) (at 238.76 132.08 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm386.pdf" (id 3) (at 241.3 129.54 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "Device:R_US") (at 152.4 121.92 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R8" (id 0) (at 152.4 116.713 90))
    (property "Value" "10" (id 1) (at 152.4 119.0244 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 152.146 122.936 90))
    (property "Datasheet" "~" (id 3) (at 152.4 121.92 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 105.41 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C17" (id 0) (at 108.331 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 108.331 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 106.3752 184.15 0))
    (property "Datasheet" "~" (id 3) (at 105.41 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 149.86 66.04 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0112" (id 0) (at 149.86 72.39 0))
    (property "Value" "GND" (id 1) (at 146.05 69.3326 0))
    (property "Footprint" "" (id 2) (at 149.86 66.04 0))
    (property "Datasheet" "" (id 3) (at 149.86 66.04 0))
    (pin "1")
  )
  (symbol (lib_id "power:+12VA") (at 222.25 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0117" (id 0) (at 222.25 53.34 0))
    (property "Value" "+12VA" (id 1) (at 222.25 45.9254 0))
    (property "Footprint" "" (id 2) (at 222.25 49.53 0))
    (property "Datasheet" "" (id 3) (at 222.25 49.53 0))
    (pin "1")
  )
  (symbol (lib_id "power:VCC") (at 82.55 41.91 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0119" (id 0) (at 82.55 45.72 0))
    (property "Value" "VCC" (id 1) (at 82.9818 37.5158 0))
    (property "Footprint" "" (id 2) (at 82.55 41.91 0))
    (property "Datasheet" "" (id 3) (at 82.55 41.91 0))
    (pin "1")
  )
  (symbol (lib_id "Regulator_Linear:AMS1117CD-1.5") (at 238.76 49.53 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U8" (id 0) (at 238.76 43.6584 0))
    (property "Value" "AMS1117-3.3" (id 1) (at 238.76 46.4335 0))
    (property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (id 2) (at 238.76 44.45 0))
    (property "Datasheet" "http://www.advanced-monolithic.com/pdf/ds1117.pdf" (id 3) (at 241.3 55.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "power:VCC") (at 72.39 25.4 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR01" (id 0) (at 72.39 29.21 0))
    (property "Value" "VCC" (id 1) (at 72.8218 21.0058 0))
    (property "Footprint" "" (id 2) (at 72.39 25.4 0))
    (property "Datasheet" "" (id 3) (at 72.39 25.4 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 209.55 102.87 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R3" (id 0) (at 208.3816 101.1428 90))
    (property "Value" "1K" (id 1) (at 210.693 101.1428 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 209.55 102.87 0))
    (property "Datasheet" "~" (id 3) (at 209.55 102.87 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 123.19 119.38 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R7" (id 0) (at 122.0216 117.6528 0))
    (property "Value" "3.3K" (id 1) (at 124.333 117.6528 0))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 123.444 118.364 90))
    (property "Datasheet" "~" (id 3) (at 123.19 119.38 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 69.85 48.26 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0120" (id 0) (at 76.2 48.26 0))
    (property "Value" "GND" (id 1) (at 74.2442 48.133 0))
    (property "Footprint" "" (id 2) (at 69.85 48.26 0))
    (property "Datasheet" "" (id 3) (at 69.85 48.26 0))
    (pin "1")
  )
  (symbol (lib_id "Connector:AudioJack3_Ground_SwitchTR") (at 190.5 129.54 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J2" (id 0) (at 195.2752 127.9144 90))
    (property "Value" "PJ325" (id 1) (at 195.2752 130.2258 90))
    (property "Footprint" "Connector_Audio:3F07_PJ307" (id 2) (at 190.5 129.54 0))
    (property "Datasheet" "~" (id 3) (at 190.5 129.54 0))
    (pin "G")
    (pin "R")
    (pin "RN")
    (pin "S")
    (pin "T")
    (pin "TN")
  )
  (symbol (lib_id "power:GND") (at 143.51 27.94 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0111" (id 0) (at 137.16 27.94 0))
    (property "Value" "GND" (id 1) (at 140.335 28.419 90))
    (property "Footprint" "" (id 2) (at 143.51 27.94 0))
    (property "Datasheet" "" (id 3) (at 143.51 27.94 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 163.83 121.92 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C4" (id 0) (at 163.83 115.5192 90))
    (property "Value" "10UF" (id 1) (at 163.83 117.8306 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 160.02 122.8852 0))
    (property "Datasheet" "~" (id 3) (at 163.83 121.92 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 146.05 128.27 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C6" (id 0) (at 146.05 121.8692 90))
    (property "Value" "200PF" (id 1) (at 146.05 124.1806 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 142.24 129.2352 0))
    (property "Datasheet" "~" (id 3) (at 146.05 128.27 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 69.85 149.86 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0124" (id 0) (at 76.2 149.86 0))
    (property "Value" "GND" (id 1) (at 74.2442 149.733 0))
    (property "Footprint" "" (id 2) (at 69.85 149.86 0))
    (property "Datasheet" "" (id 3) (at 69.85 149.86 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_US") (at 209.55 123.19 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R9" (id 0) (at 209.55 117.983 90))
    (property "Value" "10K" (id 1) (at 209.55 120.2944 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 209.296 124.206 90))
    (property "Datasheet" "~" (id 3) (at 209.55 123.19 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 109.22 110.49 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0107" (id 0) (at 109.22 116.84 0))
    (property "Value" "GND" (id 1) (at 109.22 115.0526 0))
    (property "Footprint" "" (id 2) (at 109.22 110.49 0))
    (property "Datasheet" "" (id 3) (at 109.22 110.49 0))
    (pin "1")
  )
  (symbol (lib_id "power:VCC") (at 180.34 43.18 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR04" (id 0) (at 176.53 43.18 0))
    (property "Value" "VCC" (id 1) (at 184.7342 43.6118 0))
    (property "Footprint" "" (id 2) (at 180.34 43.18 0))
    (property "Datasheet" "" (id 3) (at 180.34 43.18 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 17.78 25.4 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0128" (id 0) (at 11.43 25.4 0))
    (property "Value" "GND" (id 1) (at 13.3858 25.527 0))
    (property "Footprint" "" (id 2) (at 17.78 25.4 0))
    (property "Datasheet" "" (id 3) (at 17.78 25.4 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 17.78 76.2 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0127" (id 0) (at 11.43 76.2 0))
    (property "Value" "GND" (id 1) (at 13.3858 76.327 0))
    (property "Footprint" "" (id 2) (at 17.78 76.2 0))
    (property "Datasheet" "" (id 3) (at 17.78 76.2 0))
    (pin "1")
  )
  (symbol (lib_id "Device:CP1") (at 248.92 53.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C15" (id 0) (at 251.841 52.1716 0))
    (property "Value" "100UF" (id 1) (at 251.841 54.483 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (id 2) (at 248.92 53.34 0))
    (property "Datasheet" "~" (id 3) (at 248.92 53.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 19.05 187.96 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR014" (id 0) (at 19.05 194.31 0))
    (property "Value" "GND" (id 1) (at 19.177 192.3542 0))
    (property "Footprint" "" (id 2) (at 19.05 187.96 0))
    (property "Datasheet" "" (id 3) (at 19.05 187.96 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 48.26 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C19" (id 0) (at 51.181 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 51.181 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 49.2252 184.15 0))
    (property "Datasheet" "~" (id 3) (at 48.26 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 231.14 154.94 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP9" (id 0) (at 231.14 150.241 0))
    (property "Value" "jmp" (id 1) (at 231.14 152.5524 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 231.14 154.94 0))
    (property "Datasheet" "~" (id 3) (at 231.14 154.94 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VCC") (at 17.78 149.86 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0108" (id 0) (at 21.59 149.86 0))
    (property "Value" "VCC" (id 1) (at 13.3858 149.4282 0))
    (property "Footprint" "" (id 2) (at 17.78 149.86 0))
    (property "Datasheet" "" (id 3) (at 17.78 149.86 0))
    (pin "1")
  )
  (symbol (lib_id "power:+5VA") (at 218.44 106.68 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0104" (id 0) (at 222.25 106.68 0))
    (property "Value" "+5VA" (id 1) (at 214.884 106.68 0))
    (property "Footprint" "" (id 2) (at 218.44 106.68 0))
    (property "Datasheet" "" (id 3) (at 218.44 106.68 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 209.55 99.06 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R2" (id 0) (at 208.3816 97.3328 90))
    (property "Value" "1K" (id 1) (at 210.693 97.3328 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 209.55 99.06 0))
    (property "Datasheet" "~" (id 3) (at 209.55 99.06 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 125.73 92.71 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP4" (id 0) (at 123.19 91.1374 0))
    (property "Value" "Jumper_NO_Small" (id 1) (at 125.73 91.1375 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 125.73 92.71 0))
    (property "Datasheet" "~" (id 3) (at 125.73 92.71 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 17.78 50.8 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0126" (id 0) (at 11.43 50.8 0))
    (property "Value" "GND" (id 1) (at 13.3858 50.927 0))
    (property "Footprint" "" (id 2) (at 17.78 50.8 0))
    (property "Datasheet" "" (id 3) (at 17.78 50.8 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 82.55 48.26 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R18" (id 0) (at 87.757 48.26 90))
    (property "Value" "10K" (id 1) (at 85.4456 48.26 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 82.55 48.26 0))
    (property "Datasheet" "~" (id 3) (at 82.55 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 222.25 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0115" (id 0) (at 222.25 63.5 0))
    (property "Value" "GND" (id 1) (at 222.25 61.7126 0))
    (property "Footprint" "" (id 2) (at 222.25 57.15 0))
    (property "Datasheet" "" (id 3) (at 222.25 57.15 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_Small_US") (at 209.55 95.25 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R1" (id 0) (at 208.3816 93.5228 90))
    (property "Value" "1K" (id 1) (at 210.693 93.5228 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 209.55 95.25 0))
    (property "Datasheet" "~" (id 3) (at 209.55 95.25 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 69.85 124.46 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0123" (id 0) (at 76.2 124.46 0))
    (property "Value" "GND" (id 1) (at 74.2442 124.333 0))
    (property "Footprint" "" (id 2) (at 69.85 124.46 0))
    (property "Datasheet" "" (id 3) (at 69.85 124.46 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 96.52 148.59 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C9" (id 0) (at 96.52 142.1892 90))
    (property "Value" "2.2UF" (id 1) (at 96.52 144.5006 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 100.33 147.6248 0))
    (property "Datasheet" "~" (id 3) (at 96.52 148.59 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_POT") (at 220.98 132.08 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "RV1" (id 0) (at 219.2274 130.9116 0))
    (property "Value" "R_POT" (id 1) (at 219.2274 133.223 0))
    (property "Footprint" "cbus_288m:RV" (id 2) (at 220.98 132.08 0))
    (property "Datasheet" "~" (id 3) (at 220.98 132.08 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (symbol (lib_id "74xx:74HC164") (at 109.22 92.71 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U5" (id 0) (at 109.22 75.7894 0))
    (property "Value" "74HC164" (id 1) (at 109.22 78.5645 0))
    (property "Footprint" "Package_SO:SO-14_5.3x10.2mm_P1.27mm" (id 2) (at 132.08 100.33 0))
    (property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74HC_HCT164.pdf" (id 3) (at 132.08 100.33 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "power:VCC") (at 133.35 78.74 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0114" (id 0) (at 133.35 82.55 0))
    (property "Value" "VCC" (id 1) (at 133.7818 74.3458 0))
    (property "Footprint" "" (id 2) (at 133.35 78.74 0))
    (property "Datasheet" "" (id 3) (at 133.35 78.74 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 180.34 58.42 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR07" (id 0) (at 186.69 58.42 0))
    (property "Value" "GND" (id 1) (at 184.7342 58.293 0))
    (property "Footprint" "" (id 2) (at 180.34 58.42 0))
    (property "Datasheet" "" (id 3) (at 180.34 58.42 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 74.93 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C22" (id 0) (at 77.851 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 77.851 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 75.8952 184.15 0))
    (property "Datasheet" "~" (id 3) (at 74.93 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Oscillator:SG-8002CA") (at 195.58 27.94 0) (mirror y) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "X1" (id 0) (at 205.74 24.8159 0))
    (property "Value" "7.987M" (id 1) (at 205.74 27.3559 0))
    (property "Footprint" "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CE-4Pin_3.2x2.5mm_HandSoldering" (id 2) (at 177.8 36.83 0))
    (property "Datasheet" "https://support.epson.biz/td/api/doc_check.php?mode=dl&lang=en&Parts=SG-8002DC" (id 3) (at 198.12 27.94 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 125.73 97.79 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP6" (id 0) (at 123.19 96.2174 0))
    (property "Value" "Jumper_NO_Small" (id 1) (at 125.73 96.2175 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 125.73 97.79 0))
    (property "Datasheet" "~" (id 3) (at 125.73 97.79 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDA") (at 255.27 97.79 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0103" (id 0) (at 255.27 104.14 0))
    (property "Value" "GNDA" (id 1) (at 255.27 101.6 0))
    (property "Footprint" "" (id 2) (at 255.27 97.79 0))
    (property "Datasheet" "" (id 3) (at 255.27 97.79 0))
    (pin "1")
  )
  (symbol (lib_id "power:GND") (at 69.85 73.66 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0125" (id 0) (at 76.2 73.66 0))
    (property "Value" "GND" (id 1) (at 74.2442 73.533 0))
    (property "Footprint" "" (id 2) (at 69.85 73.66 0))
    (property "Datasheet" "" (id 3) (at 69.85 73.66 0))
    (pin "1")
  )
  (symbol (lib_id "power:GNDA") (at 96.52 186.69 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0105" (id 0) (at 96.52 193.04 0))
    (property "Value" "GNDA" (id 1) (at 96.52 191.2526 0))
    (property "Footprint" "" (id 2) (at 96.52 186.69 0))
    (property "Datasheet" "" (id 3) (at 96.52 186.69 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 146.05 152.4 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C10" (id 0) (at 146.05 145.9992 90))
    (property "Value" "200PF" (id 1) (at 146.05 148.3106 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 142.24 153.3652 0))
    (property "Datasheet" "~" (id 3) (at 146.05 152.4 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 125.73 85.09 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP1" (id 0) (at 123.19 83.5174 0))
    (property "Value" "Jumper_NO_Small" (id 1) (at 125.73 83.5175 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 125.73 85.09 0))
    (property "Datasheet" "~" (id 3) (at 125.73 85.09 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDA") (at 177.8 149.86 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0101" (id 0) (at 177.8 156.21 0))
    (property "Value" "GNDA" (id 1) (at 177.8 153.67 0))
    (property "Footprint" "" (id 2) (at 177.8 149.86 0))
    (property "Datasheet" "" (id 3) (at 177.8 149.86 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 114.3 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C23" (id 0) (at 117.221 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 117.221 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 115.2652 184.15 0))
    (property "Datasheet" "~" (id 3) (at 114.3 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Amplifier_Operational:LM2904") (at 127 179.07 0) (unit 3)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U6" (id 0) (at 125.4761 178.1615 0))
    (property "Value" "4580" (id 1) (at 125.4761 180.9366 0))
    (property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (id 2) (at 127 179.07 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm358.pdf" (id 3) (at 127 179.07 0))
    (pin "4")
    (pin "8")
  )
  (symbol (lib_id "Device:Jumper_NO_Small") (at 125.73 87.63 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP2" (id 0) (at 123.19 86.0574 0))
    (property "Value" "Jumper_NO_Small" (id 1) (at 125.73 86.0575 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm" (id 2) (at 125.73 87.63 0))
    (property "Datasheet" "~" (id 3) (at 125.73 87.63 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_Small") (at 236.22 154.94 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R16" (id 0) (at 236.22 149.9616 90))
    (property "Value" "1.2K" (id 1) (at 236.22 152.273 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 236.22 154.94 0))
    (property "Datasheet" "~" (id 3) (at 236.22 154.94 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "cbus_288m-rescue:uPD6379-Analog_DAC") (at 231.14 91.44 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U2" (id 0) (at 231.775 88.519 0))
    (property "Value" "uPD6379" (id 1) (at 231.775 90.8304 0))
    (property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (id 2) (at 240.03 91.44 0))
    (property "Datasheet" "" (id 3) (at 240.03 91.44 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
  )
  (symbol (lib_id "power:GND") (at 17.78 127 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0109" (id 0) (at 11.43 127 0))
    (property "Value" "GND" (id 1) (at 13.3858 127.127 0))
    (property "Footprint" "" (id 2) (at 17.78 127 0))
    (property "Datasheet" "" (id 3) (at 17.78 127 0))
    (pin "1")
  )
  (symbol (lib_id "Device:C") (at 96.52 124.46 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C5" (id 0) (at 96.52 118.0592 90))
    (property "Value" "2.2UF" (id 1) (at 96.52 120.3706 90))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 100.33 123.4948 0))
    (property "Datasheet" "~" (id 3) (at 96.52 124.46 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:CP1") (at 19.05 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C12" (id 0) (at 21.971 179.1716 0))
    (property "Value" "100UF" (id 1) (at 21.971 181.483 0))
    (property "Footprint" "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm" (id 2) (at 19.05 180.34 0))
    (property "Datasheet" "~" (id 3) (at 19.05 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VCC") (at 109.22 71.12 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0113" (id 0) (at 109.22 74.93 0))
    (property "Value" "VCC" (id 1) (at 105.8418 69.2658 0))
    (property "Footprint" "" (id 2) (at 109.22 71.12 0))
    (property "Datasheet" "" (id 3) (at 109.22 71.12 0))
    (pin "1")
  )
  (symbol (lib_id "Device:Jumper_NC_Small") (at 125.73 90.17 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "JP3" (id 0) (at 123.19 89.1816 0))
    (property "Value" "W" (id 1) (at 125.73 87.9117 0))
    (property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm" (id 2) (at 125.73 90.17 0))
    (property "Datasheet" "~" (id 3) (at 125.73 90.17 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R_US") (at 137.16 157.48 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R17" (id 0) (at 137.16 152.273 90))
    (property "Value" "10K" (id 1) (at 137.16 154.5844 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 136.906 158.496 90))
    (property "Datasheet" "~" (id 3) (at 137.16 157.48 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:VCC") (at 80.01 46.99 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "#PWR0121" (id 0) (at 80.01 50.8 0))
    (property "Value" "VCC" (id 1) (at 80.4418 42.5958 0))
    (property "Footprint" "" (id 2) (at 80.01 46.99 0))
    (property "Datasheet" "" (id 3) (at 80.01 46.99 0))
    (pin "1")
  )
  (symbol (lib_id "Device:R_US") (at 137.16 133.35 270) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R12" (id 0) (at 137.16 128.143 90))
    (property "Value" "10K" (id 1) (at 137.16 130.4544 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 136.906 134.366 90))
    (property "Datasheet" "~" (id 3) (at 137.16 133.35 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 66.04 180.34 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "C21" (id 0) (at 68.961 179.1716 0))
    (property "Value" "0.1UF" (id 1) (at 68.961 181.483 0))
    (property "Footprint" "Capacitor_SMD:C_0603_1608Metric" (id 2) (at 67.0052 184.15 0))
    (property "Datasheet" "~" (id 3) (at 66.04 180.34 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GNDA") (at 262.89 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR0118" (id 0) (at 262.89 63.5 0))
    (property "Value" "GNDA" (id 1) (at 262.89 61.7126 0))
    (property "Footprint" "" (id 2) (at 262.89 57.15 0))
    (property "Datasheet" "" (id 3) (at 262.89 57.15 0))
    (pin "1")
  )
  (symbol (lib_id "cbus_288m-rescue:CBUS_EDGE_CON-Audio") (at 44.45 87.63 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "J1" (id 0) (at 44.45 16.129 0))
    (property "Value" "CBUS_EDGE_CON" (id 1) (at 44.45 18.4404 0))
    (property "Footprint" "Connector_PCBEdge:CBUS_EDGE_CON" (id 2) (at 44.45 87.63 0))
    (property "Datasheet" "DOCUMENTATION" (id 3) (at 44.45 87.63 0))
    (pin "1")
    (pin "10")
    (pin "100")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "50")
    (pin "51")
    (pin "52")
    (pin "53")
    (pin "54")
    (pin "55")
    (pin "56")
    (pin "57")
    (pin "58")
    (pin "59")
    (pin "6")
    (pin "60")
    (pin "61")
    (pin "62")
    (pin "63")
    (pin "64")
    (pin "65")
    (pin "66")
    (pin "67")
    (pin "68")
    (pin "69")
    (pin "7")
    (pin "70")
    (pin "71")
    (pin "72")
    (pin "73")
    (pin "74")
    (pin "75")
    (pin "76")
    (pin "77")
    (pin "78")
    (pin "79")
    (pin "8")
    (pin "80")
    (pin "81")
    (pin "82")
    (pin "83")
    (pin "84")
    (pin "85")
    (pin "86")
    (pin "87")
    (pin "88")
    (pin "89")
    (pin "9")
    (pin "90")
    (pin "91")
    (pin "92")
    (pin "93")
    (pin "94")
    (pin "95")
    (pin "96")
    (pin "97")
    (pin "98")
    (pin "99")
  )
  (symbol (lib_id "Device:Speaker") (at 271.78 134.62 0) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "LS1" (id 0) (at 276.098 134.7216 0))
    (property "Value" "Speaker" (id 1) (at 276.098 137.033 0))
    (property "Footprint" "cbus_288m:SPEAKER" (id 2) (at 271.78 139.7 0))
    (property "Datasheet" "~" (id 3) (at 271.526 135.89 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 227.33 144.78 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 227.33 151.13 0))
    (property "Value" "GND" (id 1) (at 227.33 149.3426 0))
    (property "Footprint" "" (id 2) (at 227.33 144.78 0))
    (property "Datasheet" "" (id 3) (at 227.33 144.78 0))
    (pin "1")
  )
  (symbol (lib_id "Amplifier_Operational:LM2904") (at 137.16 146.05 0) (unit 2)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U6" (id 0) (at 137.16 137.0034 0))
    (property "Value" "4580" (id 1) (at 137.16 139.7785 0))
    (property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (id 2) (at 137.16 146.05 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm358.pdf" (id 3) (at 137.16 146.05 0))
    (pin "5")
    (pin "6")
    (pin "7")
  )
  (symbol (lib_id "Device:R_Small_US") (at 123.19 48.26 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R?" (id 0) (at 128.397 48.26 90))
    (property "Value" "10K" (id 1) (at 126.0856 48.26 90))
    (property "Footprint" "Resistor_SMD:R_0603_1608Metric" (id 2) (at 123.19 48.26 0))
    (property "Datasheet" "~" (id 3) (at 123.19 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Amplifier_Operational:LM2904") (at 137.16 121.92 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U6" (id 0) (at 137.16 112.8734 0))
    (property "Value" "4580" (id 1) (at 137.16 115.6485 0))
    (property "Footprint" "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm" (id 2) (at 137.16 121.92 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm358.pdf" (id 3) (at 137.16 121.92 0))
    (pin "1")
    (pin "2")
    (pin "3")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR01") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR02") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR04") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR05") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR06") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR07") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR013") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR014") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0101") (unit 1) (value "GNDA") (footprint "")
    )
    (path
      (reference "#PWR0103") (unit 1) (value "GNDA") (footprint "")
    )
    (path
      (reference "#PWR0104") (unit 1) (value "+5VA") (footprint "")
    )
    (path
      (reference "#PWR0105") (unit 1) (value "GNDA") (footprint "")
    )
    (path
      (reference "#PWR0106") (unit 1) (value "+5VA") (footprint "")
    )
    (path
      (reference "#PWR0107") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0108") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR0109") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0110") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0111") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0112") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0113") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR0114") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR0115") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0116") (unit 1) (value "+5VA") (footprint "")
    )
    (path
      (reference "#PWR0117") (unit 1) (value "+12VA") (footprint "")
    )
    (path
      (reference "#PWR0118") (unit 1) (value "GNDA") (footprint "")
    )
    (path
      (reference "#PWR0119") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR0120") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0121") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR0122") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0123") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0124") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0125") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0126") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0127") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR0128") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "VCC") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+12VA") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "C1") (unit 1) (value "10UF") (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A")
    )
    (path
      (reference "C2") (unit 1) (value "10UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C3") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C4") (unit 1) (value "10UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C5") (unit 1) (value "2.2UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C6") (unit 1) (value "200PF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C7") (unit 1) (value "220uf") (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm")
    )
    (path
      (reference "C8") (unit 1) (value "10UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C9") (unit 1) (value "2.2UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C10") (unit 1) (value "200PF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C11") (unit 1) (value "10UF") (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm")
    )
    (path
      (reference "C12") (unit 1) (value "100UF") (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm")
    )
    (path
      (reference "C13") (unit 1) (value "100UF") (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm")
    )
    (path
      (reference "C14") (unit 1) (value "100UF") (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm")
    )
    (path
      (reference "C15") (unit 1) (value "100UF") (footprint "Capacitor_THT:CP_Radial_D6.3mm_P2.50mm")
    )
    (path
      (reference "C16") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C17") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C18") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C19") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C20") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C21") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C22") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "C23") (unit 1) (value "0.1UF") (footprint "Capacitor_SMD:C_0603_1608Metric")
    )
    (path
      (reference "J1") (unit 1) (value "CBUS_EDGE_CON") (footprint "Connector_PCBEdge:CBUS_EDGE_CON")
    )
    (path
      (reference "J2") (unit 1) (value "PJ325") (footprint "Connector_Audio:3F07_PJ307")
    )
    (path
      (reference "JP1") (unit 1) (value "Jumper_NO_Small") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP2") (unit 1) (value "Jumper_NO_Small") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP3") (unit 1) (value "W") (footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_Pad1.0x1.5mm")
    )
    (path
      (reference "JP4") (unit 1) (value "Jumper_NO_Small") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP5") (unit 1) (value "Jumper_NO_Small") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP6") (unit 1) (value "Jumper_NO_Small") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP7") (unit 1) (value "Jumper_NO_Small") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP8") (unit 1) (value "Jumper_NO_Small") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP9") (unit 1) (value "jmp") (footprint "Jumper:SolderJumper-2_P1.3mm_Open_Pad1.0x1.5mm")
    )
    (path
      (reference "JP?") (unit 1) (value "NO") (footprint "")
    )
    (path
      (reference "L1") (unit 1) (value "10UH") (footprint "Inductor_SMD:L_1206_3216Metric")
    )
    (path
      (reference "L2") (unit 1) (value "10UH") (footprint "Inductor_SMD:L_1206_3216Metric")
    )
    (path
      (reference "LS1") (unit 1) (value "Speaker") (footprint "cbus_288m:SPEAKER")
    )
    (path
      (reference "R1") (unit 1) (value "1K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R2") (unit 1) (value "1K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R3") (unit 1) (value "1K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R4") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R5") (unit 1) (value "470") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R6") (unit 1) (value "680") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R7") (unit 1) (value "3.3K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R8") (unit 1) (value "10") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R9") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R10") (unit 1) (value "5.6K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R11") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R12") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R13") (unit 1) (value "3.3K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R14") (unit 1) (value "10") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R15") (unit 1) (value "5.6K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R16") (unit 1) (value "1.2K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R17") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R18") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R19") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R20") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "R?") (unit 1) (value "10K") (footprint "Resistor_SMD:R_0603_1608Metric")
    )
    (path
      (reference "RV1") (unit 1) (value "R_POT") (footprint "cbus_288m:RV")
    )
    (path
      (reference "U1") (unit 1) (value "YMF-288M") (footprint "Package_SO:SOIC-28W_7.5x18.7mm_P1.27mm")
    )
    (path
      (reference "U2") (unit 1) (value "uPD6379") (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm")
    )
    (path
      (reference "U3") (unit 1) (value "GAL20V8") (footprint "Package_DIP:DIP-24_W7.62mm")
    )
    (path
      (reference "U4") (unit 1) (value "74LS245") (footprint "Package_SO:SO-20_5.3x12.6mm_P1.27mm")
    )
    (path
      (reference "U5") (unit 1) (value "74HC164") (footprint "Package_SO:SO-14_5.3x10.2mm_P1.27mm")
    )
    (path
      (reference "U6") (unit 1) (value "4580") (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm")
    )
    (path
      (reference "U6") (unit 2) (value "4580") (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm")
    )
    (path
      (reference "U6") (unit 3) (value "4580") (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm")
    )
    (path
      (reference "U7") (unit 1) (value "LM386") (footprint "Package_SO:SOIC-8_5.23x5.23mm_P1.27mm")
    )
    (path
      (reference "U8") (unit 1) (value "AMS1117-3.3") (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2")
    )
    (path
      (reference "X1") (unit 1) (value "7.987M") (footprint "Oscillator:Oscillator_SMD_SeikoEpson_SG8002CE-4Pin_3.2x2.5mm_HandSoldering")
    )
  )
)
